[    0.000000] Linux version 5.14.0-529.el9.x86_64 (mockbuild@x86-64-05.build.eng.rdu2.redhat.com) (gcc (GCC) 11.5.0 20240719 (Red Hat 11.5.0-2), GNU ld version 2.35.2-56.el9) #1 SMP PREEMPT_DYNAMIC Thu Nov 14 10:13:29 EST 2024
[    0.000000] The list of certified hardware and cloud instances for Red Hat Enterprise Linux 9 can be viewed at the Red Hat Ecosystem Catalog, https://catalog.redhat.com.
[    0.000000] Command line: BOOT_IMAGE=(hd4,gpt2)/vmlinuz-5.14.0-529.el9.x86_64 root=/dev/mapper/rhel-root ro crashkernel=1G-4G:192M,4G-64G:256M,64G-:512M resume=/dev/mapper/rhel-swap rd.lvm.lv=rhel/root rd.lvm.lv=rhel/swap rhgb quiet nomodeset intel_iommu=on iommu=pt
[    0.000000] x86/tme: not enabled by BIOS
[    0.000000] x86/split lock detection: #AC: crashing the kernel on kernel split_locks and warning on user-space split_locks
[    0.000000] BIOS-provided physical RAM map:
[    0.000000] BIOS-e820: [mem 0x0000000000000000-0x000000000009ffff] usable
[    0.000000] BIOS-e820: [mem 0x00000000000a0000-0x00000000000fffff] reserved
[    0.000000] BIOS-e820: [mem 0x0000000000100000-0x0000000065bfefff] usable
[    0.000000] BIOS-e820: [mem 0x0000000065bff000-0x0000000068cfefff] reserved
[    0.000000] BIOS-e820: [mem 0x0000000068cff000-0x0000000068de9fff] ACPI data
[    0.000000] BIOS-e820: [mem 0x0000000068dea000-0x0000000068ea9fff] ACPI NVS
[    0.000000] BIOS-e820: [mem 0x0000000068eaa000-0x0000000069ffefff] reserved
[    0.000000] BIOS-e820: [mem 0x0000000069fff000-0x0000000069ffffff] usable
[    0.000000] BIOS-e820: [mem 0x000000006a000000-0x00000000787fffff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000c0000000-0x00000000cfffffff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000fe000000-0x00000000fe010fff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000fec00000-0x00000000fec00fff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000fed00000-0x00000000fed00fff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000fed20000-0x00000000fed7ffff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000fee00000-0x00000000fee00fff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000ff000000-0x00000000ffffffff] reserved
[    0.000000] BIOS-e820: [mem 0x0000000100000000-0x0000000fffffffff] usable
[    0.000000] NX (Execute Disable) protection: active
[    0.000000] APIC: Static calls initialized
[    0.000000] e820: update [mem 0x58bac018-0x58bb8c57] usable ==> usable
[    0.000000] e820: update [mem 0x58b9f018-0x58babc57] usable ==> usable
[    0.000000] e820: update [mem 0x58b6d018-0x58b9e257] usable ==> usable
[    0.000000] e820: update [mem 0x58a10018-0x58a41257] usable ==> usable
[    0.000000] extended physical RAM map:
[    0.000000] reserve setup_data: [mem 0x0000000000000000-0x000000000009ffff] usable
[    0.000000] reserve setup_data: [mem 0x00000000000a0000-0x00000000000fffff] reserved
[    0.000000] reserve setup_data: [mem 0x0000000000100000-0x0000000058a10017] usable
[    0.000000] reserve setup_data: [mem 0x0000000058a10018-0x0000000058a41257] usable
[    0.000000] reserve setup_data: [mem 0x0000000058a41258-0x0000000058b6d017] usable
[    0.000000] reserve setup_data: [mem 0x0000000058b6d018-0x0000000058b9e257] usable
[    0.000000] reserve setup_data: [mem 0x0000000058b9e258-0x0000000058b9f017] usable
[    0.000000] reserve setup_data: [mem 0x0000000058b9f018-0x0000000058babc57] usable
[    0.000000] reserve setup_data: [mem 0x0000000058babc58-0x0000000058bac017] usable
[    0.000000] reserve setup_data: [mem 0x0000000058bac018-0x0000000058bb8c57] usable
[    0.000000] reserve setup_data: [mem 0x0000000058bb8c58-0x0000000065bfefff] usable
[    0.000000] reserve setup_data: [mem 0x0000000065bff000-0x0000000068cfefff] reserved
[    0.000000] reserve setup_data: [mem 0x0000000068cff000-0x0000000068de9fff] ACPI data
[    0.000000] reserve setup_data: [mem 0x0000000068dea000-0x0000000068ea9fff] ACPI NVS
[    0.000000] reserve setup_data: [mem 0x0000000068eaa000-0x0000000069ffefff] reserved
[    0.000000] reserve setup_data: [mem 0x0000000069fff000-0x0000000069ffffff] usable
[    0.000000] reserve setup_data: [mem 0x000000006a000000-0x00000000787fffff] reserved
[    0.000000] reserve setup_data: [mem 0x00000000c0000000-0x00000000cfffffff] reserved
[    0.000000] reserve setup_data: [mem 0x00000000fe000000-0x00000000fe010fff] reserved
[    0.000000] reserve setup_data: [mem 0x00000000fec00000-0x00000000fec00fff] reserved
[    0.000000] reserve setup_data: [mem 0x00000000fed00000-0x00000000fed00fff] reserved
[    0.000000] reserve setup_data: [mem 0x00000000fed20000-0x00000000fed7ffff] reserved
[    0.000000] reserve setup_data: [mem 0x00000000fee00000-0x00000000fee00fff] reserved
[    0.000000] reserve setup_data: [mem 0x00000000ff000000-0x00000000ffffffff] reserved
[    0.000000] reserve setup_data: [mem 0x0000000100000000-0x0000000fffffffff] usable
[    0.000000] efi: EFI v2.9 by American Megatrends
[    0.000000] efi: ACPI=0x68de9000 ACPI 2.0=0x68de9014 TPMFinalLog=0x68e76000 SMBIOS=0x69b0a000 SMBIOS 3.0=0x69b09000 MEMATTR=0x5ec6d018 ESRT=0x612c4698 MOKvar=0x69b8a000 RNG=0x68d2e018 TPMEventLog=0x58bb9018 
[    0.000000] efi: Remove mem172: MMIO range=[0xc0000000-0xcfffffff] (256MB) from e820 map
[    0.000000] e820: remove [mem 0xc0000000-0xcfffffff] reserved
[    0.000000] efi: Not removing mem173: MMIO range=[0xfe000000-0xfe010fff] (68KB) from e820 map
[    0.000000] efi: Not removing mem174: MMIO range=[0xfec00000-0xfec00fff] (4KB) from e820 map
[    0.000000] efi: Not removing mem175: MMIO range=[0xfed00000-0xfed00fff] (4KB) from e820 map
[    0.000000] efi: Not removing mem177: MMIO range=[0xfee00000-0xfee00fff] (4KB) from e820 map
[    0.000000] efi: Remove mem178: MMIO range=[0xff000000-0xffffffff] (16MB) from e820 map
[    0.000000] e820: remove [mem 0xff000000-0xffffffff] reserved
[    0.000000] secureboot: Secure boot disabled
[    0.000000] SMBIOS 3.3.0 present.
[    0.000000] DMI: Lenovo ThinkEdge SE100 Planar/SB27B84845, BIOS DZE101V-1.10 11/20/2024
[    0.000000] tsc: Detected 3700.000 MHz processor
[    0.000000] tsc: Detected 3686.400 MHz TSC
[    0.000009] e820: update [mem 0x00000000-0x00000fff] usable ==> reserved
[    0.000011] e820: remove [mem 0x000a0000-0x000fffff] usable
[    0.000024] last_pfn = 0x1000000 max_arch_pfn = 0x400000000
[    0.000030] MTRR map: 6 entries (3 fixed + 3 variable; max 23), built from 10 variable MTRRs
[    0.000032] x86/PAT: Configuration [0-7]: WB  WC  UC- UC  WB  WP  UC- WT  
[    0.000487] x2apic: enabled by BIOS, switching to x2apic ops
[    0.000489] last_pfn = 0x6a000 max_arch_pfn = 0x400000000
[    0.010143] esrt: Reserving ESRT space from 0x00000000612c4698 to 0x00000000612c4748.
[    0.010153] e820: update [mem 0x612c4000-0x612c4fff] usable ==> reserved
[    0.010194] Using GB pages for direct mapping
[    0.010557] secureboot: Secure boot disabled
[    0.010558] RAMDISK: [mem 0x3fad5000-0x444abfff]
[    0.010560] ACPI: Early table checksum verification disabled
[    0.010564] ACPI: RSDP 0x0000000068DE9014 000024 (v02 LENOVO)
[    0.010568] ACPI: XSDT 0x0000000068DE8728 000164 (v01 LENOVO THINKSYS 00000100      01000013)
[    0.010574] ACPI: FACP 0x0000000068DD9000 000114 (v06 LENOVO THINKSYS 00000100      01000013)
[    0.010579] ACPI: DSDT 0x0000000068D6C000 06C6AE (v02 LENOVO THINKSYS 00000100 INTL 20210930)
[    0.010583] ACPI: FACS 0x0000000068EA7000 000040
[    0.010585] ACPI: SSDT 0x0000000068DE7000 0005FB (v02 PmRef  Cpu0Hwp  00003000 INTL 20210930)
[    0.010588] ACPI: SSDT 0x0000000068DE6000 0001AB (v02 PmRef  Cpu0Psd  00003000 INTL 20210930)
[    0.010591] ACPI: SSDT 0x0000000068DE5000 000394 (v02 PmRef  Cpu0Cst  00003001 INTL 20210930)
[    0.010593] ACPI: SSDT 0x0000000068DE3000 001620 (v02 PmRef  ApHwp    00003000 INTL 20210930)
[    0.010596] ACPI: SSDT 0x0000000068DE1000 001349 (v02 PmRef  ApPsd    00003000 INTL 20210930)
[    0.010598] ACPI: SSDT 0x0000000068DE0000 000FBB (v02 PmRef  ApCst    00003000 INTL 20210930)
[    0.010601] ACPI: SSDT 0x0000000068DDC000 003BC8 (v02 CpuRef CpuSsdt  00003000 INTL 20210930)
[    0.010603] ACPI: DTPR 0x0000000068DDB000 000088 (v01                 00000000      00000000)
[    0.010606] ACPI: SSDT 0x0000000068DDA000 00008F (v02 INTEL  PDatTabl 00001000 INTL 20210930)
[    0.010609] ACPI: FIDT 0x0000000068D6B000 00009C (v01 LENOVO THINKSYS 00000100 AMI  00010013)
[    0.010612] ACPI: OEM9 0x0000000068D6A000 000030 (v01 LNV    LNVGYERR 00000003      00000000)
[    0.010614] ACPI: SSDT 0x0000000068D69000 00038C (v02 PmaxDv Pmax_Dev 00000001 INTL 20210930)
[    0.010617] ACPI: SSDT 0x0000000068D66000 00247E (v02 INTEL  IgfxSsdt 00003000 INTL 20210930)
[    0.010619] ACPI: SSDT 0x0000000068D5C000 009B64 (v02 INTEL  TcssSsdt 00001000 INTL 20210930)
[    0.010622] ACPI: HPET 0x0000000068D5B000 000038 (v01 LENOVO THINKSYS 00000100      01000013)
[    0.010624] ACPI: APIC 0x0000000068D5A000 000358 (v05 LENOVO THINKSYS 00000100      01000013)
[    0.010627] ACPI: MCFG 0x0000000068D59000 00003C (v01 LENOVO THINKSYS 00000100      01000013)
[    0.010629] ACPI: SSDT 0x0000000068D4E000 00ABCE (v02 LENOVO MtlP_Rvp 00001000 INTL 20210930)
[    0.010632] ACPI: SSDT 0x0000000068D4C000 00147F (v02 LENOVO I2Pm_Rvp 00001000 INTL 20210930)
[    0.010634] ACPI: UEFI 0x0000000068E5E000 000048 (v01 LENOVO THINKSYS 00000100      01000013)
[    0.010637] ACPI: NHLT 0x0000000068D47000 00002D (v00 LENOVO THINKSYS 00000100      01000013)
[    0.010639] ACPI: LPIT 0x0000000068D46000 0000CC (v01 LENOVO THINKSYS 00000100      01000013)
[    0.010642] ACPI: SSDT 0x0000000068D44000 000CA6 (v02 LENOVO PtidDevc 00001000 INTL 20210930)
[    0.010644] ACPI: SSDT 0x0000000068D3E000 005E42 (v02 LENOVO TbtTypeC 00000000 INTL 20210930)
[    0.010647] ACPI: DBGP 0x0000000068D3D000 000034 (v01 LENOVO THINKSYS 00000100      01000013)
[    0.010649] ACPI: DBG2 0x0000000068D3C000 000054 (v00 LENOVO THINKSYS 00000100      01000013)
[    0.010652] ACPI: SSDT 0x0000000068D3A000 00115C (v02 LENOVO UsbCTabl 00001000 INTL 20210930)
[    0.010654] ACPI: DMAR 0x0000000068D39000 000098 (v01 LENOVO THINKSYS 00000100      01000013)
[    0.010657] ACPI: FPDT 0x0000000068D38000 000044 (v01 LENOVO THINKSYS 00000100      01000013)
[    0.010659] ACPI: SSDT 0x0000000068D35000 00281A (v02 SocGpe SocGpe   00003000 INTL 20210930)
[    0.010662] ACPI: SSDT 0x0000000068D32000 0028D3 (v02 SocCmn SocCmn   00003000 INTL 20210930)
[    0.010664] ACPI: SPCR 0x0000000068D31000 000050 (v02 LENOVO THINKSYS 00000100      00050020)
[    0.010666] ACPI: TPM2 0x0000000068D2F000 00004C (v04 LENOVO THINKSYS 00000001 AMI  00000000)
[    0.010669] ACPI: SLIC 0x0000000068D4B000 000176 (v01 LENOVO THINKSYS 00000100 AMI  00010013)
[    0.010671] ACPI: PHAT 0x0000000068D4A000 000A1F (v01 LENOVO THINKSYS 00000005 MSFT 0100000D)
[    0.010674] ACPI: ASF! 0x0000000068D49000 000074 (v32 LENOVO THINKSYS 00000100      01000013)
[    0.010677] ACPI: SSDT 0x0000000068D48000 000313 (v02 LENOVO CDNTABLE 00001000 INTL 20210930)
[    0.010679] ACPI: SSDT 0x0000000068D30000 000623 (v02 LENOVO THINKSYS 00000000 INTL 20210930)
[    0.010682] ACPI: WSMT 0x0000000068D45000 000028 (v01 LENOVO THINKSYS 00000100 AMI  00010013)
[    0.010684] ACPI: Reserving FACP table memory at [mem 0x68dd9000-0x68dd9113]
[    0.010685] ACPI: Reserving DSDT table memory at [mem 0x68d6c000-0x68dd86ad]
[    0.010687] ACPI: Reserving FACS table memory at [mem 0x68ea7000-0x68ea703f]
[    0.010687] ACPI: Reserving SSDT table memory at [mem 0x68de7000-0x68de75fa]
[    0.010688] ACPI: Reserving SSDT table memory at [mem 0x68de6000-0x68de61aa]
[    0.010689] ACPI: Reserving SSDT table memory at [mem 0x68de5000-0x68de5393]
[    0.010690] ACPI: Reserving SSDT table memory at [mem 0x68de3000-0x68de461f]
[    0.010691] ACPI: Reserving SSDT table memory at [mem 0x68de1000-0x68de2348]
[    0.010692] ACPI: Reserving SSDT table memory at [mem 0x68de0000-0x68de0fba]
[    0.010693] ACPI: Reserving SSDT table memory at [mem 0x68ddc000-0x68ddfbc7]
[    0.010693] ACPI: Reserving DTPR table memory at [mem 0x68ddb000-0x68ddb087]
[    0.010694] ACPI: Reserving SSDT table memory at [mem 0x68dda000-0x68dda08e]
[    0.010695] ACPI: Reserving FIDT table memory at [mem 0x68d6b000-0x68d6b09b]
[    0.010696] ACPI: Reserving OEM9 table memory at [mem 0x68d6a000-0x68d6a02f]
[    0.010697] ACPI: Reserving SSDT table memory at [mem 0x68d69000-0x68d6938b]
[    0.010698] ACPI: Reserving SSDT table memory at [mem 0x68d66000-0x68d6847d]
[    0.010698] ACPI: Reserving SSDT table memory at [mem 0x68d5c000-0x68d65b63]
[    0.010699] ACPI: Reserving HPET table memory at [mem 0x68d5b000-0x68d5b037]
[    0.010700] ACPI: Reserving APIC table memory at [mem 0x68d5a000-0x68d5a357]
[    0.010701] ACPI: Reserving MCFG table memory at [mem 0x68d59000-0x68d5903b]
[    0.010702] ACPI: Reserving SSDT table memory at [mem 0x68d4e000-0x68d58bcd]
[    0.010702] ACPI: Reserving SSDT table memory at [mem 0x68d4c000-0x68d4d47e]
[    0.010703] ACPI: Reserving UEFI table memory at [mem 0x68e5e000-0x68e5e047]
[    0.010704] ACPI: Reserving NHLT table memory at [mem 0x68d47000-0x68d4702c]
[    0.010705] ACPI: Reserving LPIT table memory at [mem 0x68d46000-0x68d460cb]
[    0.010706] ACPI: Reserving SSDT table memory at [mem 0x68d44000-0x68d44ca5]
[    0.010706] ACPI: Reserving SSDT table memory at [mem 0x68d3e000-0x68d43e41]
[    0.010707] ACPI: Reserving DBGP table memory at [mem 0x68d3d000-0x68d3d033]
[    0.010708] ACPI: Reserving DBG2 table memory at [mem 0x68d3c000-0x68d3c053]
[    0.010709] ACPI: Reserving SSDT table memory at [mem 0x68d3a000-0x68d3b15b]
[    0.010710] ACPI: Reserving DMAR table memory at [mem 0x68d39000-0x68d39097]
[    0.010710] ACPI: Reserving FPDT table memory at [mem 0x68d38000-0x68d38043]
[    0.010711] ACPI: Reserving SSDT table memory at [mem 0x68d35000-0x68d37819]
[    0.010712] ACPI: Reserving SSDT table memory at [mem 0x68d32000-0x68d348d2]
[    0.010713] ACPI: Reserving SPCR table memory at [mem 0x68d31000-0x68d3104f]
[    0.010714] ACPI: Reserving TPM2 table memory at [mem 0x68d2f000-0x68d2f04b]
[    0.010715] ACPI: Reserving SLIC table memory at [mem 0x68d4b000-0x68d4b175]
[    0.010715] ACPI: Reserving PHAT table memory at [mem 0x68d4a000-0x68d4aa1e]
[    0.010716] ACPI: Reserving ASF! table memory at [mem 0x68d49000-0x68d49073]
[    0.010717] ACPI: Reserving SSDT table memory at [mem 0x68d48000-0x68d48312]
[    0.010718] ACPI: Reserving SSDT table memory at [mem 0x68d30000-0x68d30622]
[    0.010719] ACPI: Reserving WSMT table memory at [mem 0x68d45000-0x68d45027]
[    0.010771] APIC: Switched APIC routing to: cluster x2apic
[    0.010951] No NUMA configuration found
[    0.010952] Faking a node at [mem 0x0000000000000000-0x0000000fffffffff]
[    0.010961] NODE_DATA(0) allocated [mem 0xffffd5000-0xfffffffff]
[    0.011185] Reserving 256MB of memory at 752MB for crashkernel (System RAM: 63067MB)
[    0.011258] Zone ranges:
[    0.011259]   DMA      [mem 0x0000000000001000-0x0000000000ffffff]
[    0.011261]   DMA32    [mem 0x0000000001000000-0x00000000ffffffff]
[    0.011263]   Normal   [mem 0x0000000100000000-0x0000000fffffffff]
[    0.011265]   Device   empty
[    0.011266] Movable zone start for each node
[    0.011268] Early memory node ranges
[    0.011268]   node   0: [mem 0x0000000000001000-0x000000000009ffff]
[    0.011270]   node   0: [mem 0x0000000000100000-0x0000000065bfefff]
[    0.011271]   node   0: [mem 0x0000000069fff000-0x0000000069ffffff]
[    0.011272]   node   0: [mem 0x0000000100000000-0x0000000fffffffff]
[    0.011277] Initmem setup node 0 [mem 0x0000000000001000-0x0000000fffffffff]
[    0.011284] On node 0, zone DMA: 1 pages in unavailable ranges
[    0.011318] On node 0, zone DMA: 96 pages in unavailable ranges
[    0.014465] On node 0, zone DMA32: 17408 pages in unavailable ranges
[    0.014918] On node 0, zone Normal: 24576 pages in unavailable ranges
[    0.015274] ACPI: PM-Timer IO Port: 0x1808
[    0.015285] ACPI: X2APIC_NMI (uid[0xffffffff] high level lint[0x1])
[    0.015320] IOAPIC[0]: apic_id 2, version 32, address 0xfec00000, GSI 0-119
[    0.015324] ACPI: INT_SRC_OVR (bus 0 bus_irq 0 global_irq 2 dfl dfl)
[    0.015326] ACPI: INT_SRC_OVR (bus 0 bus_irq 9 global_irq 9 high level)
[    0.015331] ACPI: Using ACPI (MADT) for SMP configuration information
[    0.015332] ACPI: HPET id: 0x8086a201 base: 0xfed00000
[    0.015337] ACPI: SPCR: console: uart,io,0x3f8,115200
[    0.015339] TSC deadline timer available
[    0.015342] CPU topo: Max. logical packages:   1
[    0.015343] CPU topo: Max. logical dies:       1
[    0.015343] CPU topo: Max. dies per package:   1
[    0.015346] CPU topo: Max. threads per core:   1
[    0.015347] CPU topo: Num. cores per package:    14
[    0.015348] CPU topo: Num. threads per package:  14
[    0.015348] CPU topo: Allowing 14 present CPUs plus 0 hotplug CPUs
[    0.015374] PM: hibernation: Registered nosave memory: [mem 0x00000000-0x00000fff]
[    0.015376] PM: hibernation: Registered nosave memory: [mem 0x000a0000-0x000fffff]
[    0.015378] PM: hibernation: Registered nosave memory: [mem 0x58a10000-0x58a10fff]
[    0.015380] PM: hibernation: Registered nosave memory: [mem 0x58a41000-0x58a41fff]
[    0.015381] PM: hibernation: Registered nosave memory: [mem 0x58b6d000-0x58b6dfff]
[    0.015382] PM: hibernation: Registered nosave memory: [mem 0x58b9e000-0x58b9efff]
[    0.015383] PM: hibernation: Registered nosave memory: [mem 0x58b9f000-0x58b9ffff]
[    0.015385] PM: hibernation: Registered nosave memory: [mem 0x58bab000-0x58babfff]
[    0.015385] PM: hibernation: Registered nosave memory: [mem 0x58bac000-0x58bacfff]
[    0.015387] PM: hibernation: Registered nosave memory: [mem 0x58bb8000-0x58bb8fff]
[    0.015389] PM: hibernation: Registered nosave memory: [mem 0x612c4000-0x612c4fff]
[    0.015390] PM: hibernation: Registered nosave memory: [mem 0x65bff000-0x68cfefff]
[    0.015391] PM: hibernation: Registered nosave memory: [mem 0x68cff000-0x68de9fff]
[    0.015392] PM: hibernation: Registered nosave memory: [mem 0x68dea000-0x68ea9fff]
[    0.015393] PM: hibernation: Registered nosave memory: [mem 0x68eaa000-0x69ffefff]
[    0.015394] PM: hibernation: Registered nosave memory: [mem 0x6a000000-0x787fffff]
[    0.015395] PM: hibernation: Registered nosave memory: [mem 0x78800000-0xfdffffff]
[    0.015396] PM: hibernation: Registered nosave memory: [mem 0xfe000000-0xfe010fff]
[    0.015397] PM: hibernation: Registered nosave memory: [mem 0xfe011000-0xfebfffff]
[    0.015397] PM: hibernation: Registered nosave memory: [mem 0xfec00000-0xfec00fff]
[    0.015398] PM: hibernation: Registered nosave memory: [mem 0xfec01000-0xfecfffff]
[    0.015399] PM: hibernation: Registered nosave memory: [mem 0xfed00000-0xfed00fff]
[    0.015399] PM: hibernation: Registered nosave memory: [mem 0xfed01000-0xfed1ffff]
[    0.015400] PM: hibernation: Registered nosave memory: [mem 0xfed20000-0xfed7ffff]
[    0.015401] PM: hibernation: Registered nosave memory: [mem 0xfed80000-0xfedfffff]
[    0.015401] PM: hibernation: Registered nosave memory: [mem 0xfee00000-0xfee00fff]
[    0.015402] PM: hibernation: Registered nosave memory: [mem 0xfee01000-0xffffffff]
[    0.015404] [mem 0x78800000-0xfdffffff] available for PCI devices
[    0.015407] Booting paravirtualized kernel on bare hardware
[    0.015410] clocksource: refined-jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 1910969940391419 ns
[    0.022978] setup_percpu: NR_CPUS:8192 nr_cpumask_bits:14 nr_cpu_ids:14 nr_node_ids:1
[    0.023547] percpu: Embedded 64 pages/cpu s225280 r8192 d28672 u262144
[    0.023553] pcpu-alloc: s225280 r8192 d28672 u262144 alloc=1*2097152
[    0.023556] pcpu-alloc: [0] 00 01 02 03 04 05 06 07 [0] 08 09 10 11 12 13 -- -- 
[    0.023581] Kernel command line: BOOT_IMAGE=(hd4,gpt2)/vmlinuz-5.14.0-529.el9.x86_64 root=/dev/mapper/rhel-root ro crashkernel=1G-4G:192M,4G-64G:256M,64G-:512M resume=/dev/mapper/rhel-swap rd.lvm.lv=rhel/root rd.lvm.lv=rhel/swap rhgb quiet nomodeset intel_iommu=on iommu=pt
[    0.023726] Booted with the nomodeset parameter. Only the system framebuffer will be available
[    0.023743] DMAR: IOMMU enabled
[    0.023761] Unknown kernel command line parameters "rhgb BOOT_IMAGE=(hd4,gpt2)/vmlinuz-5.14.0-529.el9.x86_64", will be passed to user space.
[    0.023788] random: crng init done
[    0.029340] Dentry cache hash table entries: 8388608 (order: 14, 67108864 bytes, linear)
[    0.032135] Inode-cache hash table entries: 4194304 (order: 13, 33554432 bytes, linear)
[    0.032332] Fallback order for Node 0: 0 
[    0.032336] Built 1 zonelists, mobility grouping on.  Total pages: 15892880
[    0.032337] Policy zone: Normal
[    0.032540] mem auto-init: stack:off, heap alloc:off, heap free:off
[    0.032551] software IO TLB: area num 16.
[    0.060408] Memory: 1186988K/64581244K available (16384K kernel code, 5733K rwdata, 13184K rodata, 4020K init, 5500K bss, 1778884K reserved, 0K cma-reserved)
[    0.060685] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=14, Nodes=1
[    0.060712] ftrace: allocating 48683 entries in 191 pages
[    0.070073] ftrace: allocated 191 pages with 7 groups
[    0.070910] Dynamic Preempt: voluntary
[    0.070986] rcu: Preemptible hierarchical RCU implementation.
[    0.070987] rcu: 	RCU event tracing is enabled.
[    0.070988] rcu: 	RCU restricting CPUs from NR_CPUS=8192 to nr_cpu_ids=14.
[    0.070990] 	Trampoline variant of Tasks RCU enabled.
[    0.070990] 	Rude variant of Tasks RCU enabled.
[    0.070991] 	Tracing variant of Tasks RCU enabled.
[    0.070992] rcu: RCU calculated value of scheduler-enlistment delay is 100 jiffies.
[    0.070993] rcu: Adjusting geometry for rcu_fanout_leaf=16, nr_cpu_ids=14
[    0.071005] RCU Tasks: Setting shift to 4 and lim to 1 rcu_task_cb_adjust=1.
[    0.071008] RCU Tasks Rude: Setting shift to 4 and lim to 1 rcu_task_cb_adjust=1.
[    0.071009] RCU Tasks Trace: Setting shift to 4 and lim to 1 rcu_task_cb_adjust=1.
[    0.075050] NR_IRQS: 524544, nr_irqs: 2168, preallocated irqs: 16
[    0.075331] rcu: srcu_init: Setting srcu_struct sizes based on contention.
[    0.075624] kfence: initialized - using 2097152 bytes for 255 objects at 0x(____ptrval____)-0x(____ptrval____)
[    0.075667] Console: colour dummy device 80x25
[    0.075670] printk: legacy console [tty0] enabled
[    0.075720] ACPI: Core revision 20230331
[    0.076288] hpet: HPET dysfunctional in PC10. Force disabled.
[    0.076290] APIC: Switch to symmetric I/O mode setup
[    0.076292] DMAR: Host address width 42
[    0.076293] DMAR: DRHD base: 0x000000fc800000 flags: 0x0
[    0.076302] DMAR: dmar0: reg_base_addr fc800000 ver 7:0 cap c9de008cee690462 ecap 12ca9a00f0ef5e
[    0.076305] DMAR: DRHD base: 0x000000fc801000 flags: 0x1
[    0.076310] DMAR: dmar1: reg_base_addr fc801000 ver 7:0 cap c9de008cee690462 ecap 12ca9a00f0efde
[    0.076313] DMAR: SATC flags: 0x1
[    0.076315] DMAR-IR: IOAPIC id 2 under DRHD base  0xfc801000 IOMMU 1
[    0.076317] DMAR-IR: HPET id 0 under DRHD base 0xfc801000
[    0.076318] DMAR-IR: Queued invalidation will be enabled to support x2apic and Intr-remapping.
[    0.077994] DMAR-IR: Enabled IRQ remapping in x2apic mode
[    0.082116] clocksource: tsc-early: mask: 0xffffffffffffffff max_cycles: 0x6a464ae9873, max_idle_ns: 881590529744 ns
[    0.082124] Calibrating delay loop (skipped), value calculated using timer frequency.. 7372.80 BogoMIPS (lpj=3686400)
[    0.082198] CPU0: Thermal monitoring enabled (TM1)
[    0.082201] x86/cpu: User Mode Instruction Prevention (UMIP) activated
[    0.082409] process: using mwait in idle threads
[    0.082411] Last level iTLB entries: 4KB 0, 2MB 0, 4MB 0
[    0.082412] Last level dTLB entries: 4KB 0, 2MB 0, 4MB 0, 1GB 0
[    0.082416] Spectre V1 : Mitigation: usercopy/swapgs barriers and __user pointer sanitization
[    0.082419] Spectre V2 : Mitigation: Enhanced / Automatic IBRS
[    0.082420] Spectre V2 : Spectre v2 / SpectreRSB mitigation: Filling RSB on context switch
[    0.082422] Spectre V2 : mitigation: Enabling conditional Indirect Branch Prediction Barrier
[    0.082424] Speculative Store Bypass: Mitigation: Speculative Store Bypass disabled via prctl
[    0.082435] x86/fpu: Supporting XSAVE feature 0x001: 'x87 floating point registers'
[    0.082437] x86/fpu: Supporting XSAVE feature 0x002: 'SSE registers'
[    0.082438] x86/fpu: Supporting XSAVE feature 0x004: 'AVX registers'
[    0.082438] x86/fpu: Supporting XSAVE feature 0x200: 'Protection Keys User registers'
[    0.082439] x86/fpu: Supporting XSAVE feature 0x800: 'Control-flow User registers'
[    0.082441] x86/fpu: xstate_offset[2]:  576, xstate_sizes[2]:  256
[    0.082442] x86/fpu: xstate_offset[9]:  832, xstate_sizes[9]:    8
[    0.082443] x86/fpu: xstate_offset[11]:  840, xstate_sizes[11]:   16
[    0.082445] x86/fpu: Enabled xstate features 0xa07, context size is 856 bytes, using 'compacted' format.
[    0.083121] Freeing SMP alternatives memory: 40K
[    0.083121] pid_max: default: 32768 minimum: 301
[    0.083121] LSM: initializing lsm=lockdown,capability,yama,integrity,selinux,bpf
[    0.083121] Yama: becoming mindful.
[    0.083121] SELinux:  Initializing.
[    0.083121] LSM support for eBPF active
[    0.083121] Mount-cache hash table entries: 131072 (order: 8, 1048576 bytes, linear)
[    0.083121] Mountpoint-cache hash table entries: 131072 (order: 8, 1048576 bytes, linear)
[    0.083121] smpboot: CPU0: Genuine Intel(R) 0000 (family: 0x6, model: 0xc5, stepping: 0x2)
[    0.083121] Performance Events: XSAVE Architectural LBR, PEBS fmt4+-baseline,  AnyThread deprecated, generic architected perfmon, 32-deep LBR, full-width counters, Intel PMU driver.
[    0.083121] ... version:                5
[    0.083121] ... bit width:              48
[    0.083121] ... generic registers:      8
[    0.083121] ... value mask:             0000ffffffffffff
[    0.083121] ... max period:             00007fffffffffff
[    0.083121] ... fixed-purpose events:   3
[    0.083121] ... event mask:             00010007000000ff
[    0.083121] signal: max sigframe size: 3632
[    0.083121] Estimated ratio of average max frequency by base frequency (times 1024): 1024
[    0.083121] rcu: Hierarchical SRCU implementation.
[    0.083121] rcu: 	Max phase no-delay instances is 400.
[    0.083529] NMI watchdog: Enabled. Permanently consumes one hw-PMU counter.
[    0.083641] smp: Bringing up secondary CPUs ...
[    0.083724] smpboot: x86: Booting SMP configuration:
[    0.083726] .... node  #0, CPUs:        #1  #2  #3  #4  #5  #6  #7  #8  #9 #10 #11 #12 #13
[    0.091254] smp: Brought up 1 node, 14 CPUs
[    0.091254] smpboot: Total of 14 processors activated (103219.20 BogoMIPS)
[    0.132167] node 0 deferred pages initialised in 40ms
[    0.134689] devtmpfs: initialized
[    0.134689] x86/mm: Memory block size: 2048MB
[    0.135258] ACPI: PM: Registering ACPI NVS region [mem 0x68dea000-0x68ea9fff] (786432 bytes)
[    0.135258] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 1911260446275000 ns
[    0.135258] futex hash table entries: 4096 (order: 6, 262144 bytes, linear)
[    0.135299] pinctrl core: initialized pinctrl subsystem
[    0.135782] NET: Registered PF_NETLINK/PF_ROUTE protocol family
[    0.135906] DMA: preallocated 4096 KiB GFP_KERNEL pool for atomic allocations
[    0.135912] DMA: preallocated 4096 KiB GFP_KERNEL|GFP_DMA pool for atomic allocations
[    0.135915] DMA: preallocated 4096 KiB GFP_KERNEL|GFP_DMA32 pool for atomic allocations
[    0.135930] audit: initializing netlink subsys (disabled)
[    0.136131] audit: type=2000 audit(1732870234.054:1): state=initialized audit_enabled=0 res=1
[    0.136215] thermal_sys: Registered thermal governor 'fair_share'
[    0.136217] thermal_sys: Registered thermal governor 'step_wise'
[    0.136218] thermal_sys: Registered thermal governor 'user_space'
[    0.136226] cpuidle: using governor menu
[    0.136226] acpiphp: ACPI Hot Plug PCI Controller Driver version: 0.5
[    0.136270] PCI: ECAM [mem 0xc0000000-0xcfffffff] (base 0xc0000000) for domain 0000 [bus 00-ff]
[    0.136289] PCI: Using configuration type 1 for base access
[    0.138308] kprobes: kprobe jump-optimization is enabled. All kprobes are optimized if possible.
[    0.138308] HugeTLB: registered 1.00 GiB page size, pre-allocated 0 pages
[    0.138308] HugeTLB: 16380 KiB vmemmap can be freed for a 1.00 GiB page
[    0.138308] HugeTLB: registered 2.00 MiB page size, pre-allocated 0 pages
[    0.138308] HugeTLB: 28 KiB vmemmap can be freed for a 2.00 MiB page
[    0.138325] Demotion targets for Node 0: null
[    0.138325] cryptd: max_cpu_qlen set to 1000
[    0.138325] ACPI: Added _OSI(Module Device)
[    0.138325] ACPI: Added _OSI(Processor Device)
[    0.138325] ACPI: Added _OSI(3.0 _SCP Extensions)
[    0.138325] ACPI: Added _OSI(Processor Aggregator Device)
[    0.228945] ACPI: 21 ACPI AML tables successfully acquired and loaded
[    0.241141] ACPI: _OSC evaluated successfully for all CPUs
[    0.242823] ACPI: Interpreter enabled
[    0.242884] ACPI: PM: (supports S0 S5)
[    0.242885] ACPI: Using IOAPIC for interrupt routing
[    0.244714] PCI: Using host bridge windows from ACPI; if necessary, use "pci=nocrs" and report a bug
[    0.244716] PCI: Ignoring E820 reservations for host bridge windows
[    0.246584] ACPI: Enabled 11 GPEs in block 00 to 7F
[    0.246606] ACPI: Enabled 8 GPEs in block 80 to DF
[    0.249389] ACPI: \_SB_.PC00.RP12.PXP_: New power resource
[    0.250520] ACPI: \_SB_.PC00.RP09.PXP_: New power resource
[    0.251688] ACPI: \_SB_.PC00.RP10.PXP_: New power resource
[    0.252884] ACPI: \_SB_.PC00.RP11.PXP_: New power resource
[    0.254065] ACPI: \_SB_.PC00.RP01.PXP_: New power resource
[    0.257680] ACPI: \_SB_.PC00.RP06.PXP_: New power resource
[    0.258911] ACPI: \_SB_.PC00.RP07.PXP_: New power resource
[    0.292360] ACPI: \_SB_.PC00.D3C_: New power resource
[    0.299710] ACPI: \_SB_.PC00.PAUD: New power resource
[    0.304923] ACPI: \PIN_: New power resource
[    0.305317] ACPI: PCI Root Bridge [PC00] (domain 0000 [bus 00-fe])
[    0.305326] acpi PNP0A08:00: _OSC: OS supports [ExtendedConfig ASPM ClockPM Segments MSI EDR HPX-Type3]
[    0.306950] acpi PNP0A08:00: _OSC: OS now controls [PCIeHotplug SHPCHotplug PME AER PCIeCapability LTR DPC]
[    0.308952] PCI host bridge to bus 0000:00
[    0.308956] pci_bus 0000:00: root bus resource [io  0x0000-0x0cf7 window]
[    0.308959] pci_bus 0000:00: root bus resource [io  0x0d00-0xffff window]
[    0.308960] pci_bus 0000:00: root bus resource [mem 0x000a0000-0x000bffff window]
[    0.308961] pci_bus 0000:00: root bus resource [mem 0x80000000-0xbfffffff window]
[    0.308963] pci_bus 0000:00: root bus resource [mem 0x4000000000-0x3ffbfffffff window]
[    0.308964] pci_bus 0000:00: root bus resource [bus 00-fe]
[    0.420777] pci 0000:00:00.0: [8086:7d20] type 00 class 0x060000 conventional PCI endpoint
[    0.420989] pci 0000:00:01.0: [8086:7ecc] type 01 class 0x060400 PCIe Root Port
[    0.421023] pci 0000:00:01.0: PCI bridge to [bus 01]
[    0.421066] pci 0000:00:01.0: broken device, retraining non-functional downstream link at 2.5GT/s
[    0.463195] pci 0000:00:01.0: PME# supported from D0 D3hot D3cold
[    0.463232] pci 0000:00:01.0: PTM enabled (root), 4ns granularity
[    0.463395] pci 0000:00:02.0: [8086:7d51] type 00 class 0x030000 PCIe Root Complex Integrated Endpoint
[    0.463418] pci 0000:00:02.0: BAR 0 [mem 0x4017000000-0x4017ffffff 64bit pref]
[    0.463434] pci 0000:00:02.0: BAR 2 [mem 0x4000000000-0x400fffffff 64bit pref]
[    0.463485] pci 0000:00:02.0: DMAR: Skip IOMMU disabling for graphics
[    0.463490] pci 0000:00:02.0: Video device with shadowed ROM at [mem 0x000c0000-0x000dffff]
[    0.463545] pci 0000:00:02.0: PME# supported from D0 D3hot
[    0.463569] pci 0000:00:02.0: VF BAR 0 [mem 0x4010000000-0x4010ffffff 64bit pref]
[    0.463570] pci 0000:00:02.0: VF BAR 0 [mem 0x4010000000-0x4016ffffff 64bit pref]: contains BAR 0 for 7 VFs
[    0.463821] pci 0000:00:06.0: [8086:7eca] type 01 class 0x060400 PCIe Root Port
[    0.463862] pci 0000:00:06.0: PCI bridge to [bus 02]
[    0.463871] pci 0000:00:06.0:   bridge window [mem 0x81500000-0x815fffff]
[    0.463976] pci 0000:00:06.0: PME# supported from D0 D3hot D3cold
[    0.464019] pci 0000:00:06.0: PTM enabled (root), 4ns granularity
[    0.464223] pci 0000:00:06.2: [8086:7ecb] type 01 class 0x060400 PCIe Root Port
[    0.464260] pci 0000:00:06.2: PCI bridge to [bus 03]
[    0.464267] pci 0000:00:06.2:   bridge window [mem 0x81400000-0x814fffff]
[    0.464371] pci 0000:00:06.2: PME# supported from D0 D3hot D3cold
[    0.464413] pci 0000:00:06.2: PTM enabled (root), 4ns granularity
[    0.464619] pci 0000:00:08.0: [8086:774c] type 00 class 0x088000 conventional PCI endpoint
[    0.464645] pci 0000:00:08.0: BAR 0 [mem 0x4028068000-0x4028068fff 64bit]
[    0.464810] pci 0000:00:0a.0: [8086:7d0d] type 00 class 0x118000 PCIe Root Complex Integrated Endpoint
[    0.464824] pci 0000:00:0a.0: BAR 0 [mem 0x4028000000-0x402803ffff 64bit]
[    0.464855] pci 0000:00:0a.0: enabling Extended Tags
[    0.464954] pci 0000:00:0b.0: [8086:7d1d] type 00 class 0x120000 PCIe Root Complex Integrated Endpoint
[    0.464970] pci 0000:00:0b.0: BAR 0 [mem 0x4020000000-0x4027ffffff 64bit]
[    0.464990] pci 0000:00:0b.0: BAR 4 [mem 0x4028067000-0x4028067fff 64bit]
[    0.465137] pci 0000:00:0d.0: [8086:7ec0] type 00 class 0x0c0330 conventional PCI endpoint
[    0.465159] pci 0000:00:0d.0: BAR 0 [mem 0x4028050000-0x402805ffff 64bit]
[    0.465250] pci 0000:00:0d.0: PME# supported from D3hot D3cold
[    0.465717] pci 0000:00:14.0: [8086:777d] type 00 class 0x0c0330 conventional PCI endpoint
[    0.465739] pci 0000:00:14.0: BAR 0 [mem 0x4028040000-0x402804ffff 64bit]
[    0.465828] pci 0000:00:14.0: PME# supported from D3hot D3cold
[    0.466275] pci 0000:00:14.2: [8086:777f] type 00 class 0x050000 conventional PCI endpoint
[    0.466298] pci 0000:00:14.2: BAR 0 [mem 0x4028060000-0x4028063fff 64bit]
[    0.466313] pci 0000:00:14.2: BAR 2 [mem 0x4028066000-0x4028066fff 64bit]
[    0.466450] pci 0000:00:16.0: [8086:7770] type 00 class 0x078000 conventional PCI endpoint
[    0.466476] pci 0000:00:16.0: BAR 0 [mem 0x4028065000-0x4028065fff 64bit]
[    0.466579] pci 0000:00:16.0: PME# supported from D3hot
[    0.467185] pci 0000:00:16.3: [8086:7773] type 00 class 0x070002 conventional PCI endpoint
[    0.467206] pci 0000:00:16.3: BAR 0 [io  0x4020-0x4027]
[    0.467216] pci 0000:00:16.3: BAR 1 [mem 0x81600000-0x81600fff]
[    0.467404] pci 0000:00:1c.0: [8086:773c] type 01 class 0x060400 PCIe Root Port
[    0.467437] pci 0000:00:1c.0: PCI bridge to [bus 04]
[    0.467443] pci 0000:00:1c.0:   bridge window [mem 0x81300000-0x813fffff]
[    0.467455] pci 0000:00:1c.0:   bridge window [mem 0x4018000000-0x40180fffff 64bit pref]
[    0.467532] pci 0000:00:1c.0: PME# supported from D0 D3hot D3cold
[    0.467566] pci 0000:00:1c.0: PTM enabled (root), 4ns granularity
[    0.467702] pci 0000:00:1c.6: [8086:773e] type 01 class 0x060400 PCIe Root Port
[    0.467735] pci 0000:00:1c.6: PCI bridge to [bus 05-06]
[    0.467739] pci 0000:00:1c.6:   bridge window [io  0x3000-0x3fff]
[    0.467742] pci 0000:00:1c.6:   bridge window [mem 0x80000000-0x812fffff]
[    0.467831] pci 0000:00:1c.6: PME# supported from D0 D3hot D3cold
[    0.467862] pci 0000:00:1c.6: PTM enabled (root), 4ns granularity
[    0.467991] pci 0000:00:1f.0: [8086:7701] type 00 class 0x060100 conventional PCI endpoint
[    0.468423] pci 0000:00:1f.4: [8086:7722] type 00 class 0x0c0500 conventional PCI endpoint
[    0.468450] pci 0000:00:1f.4: BAR 0 [mem 0x4028064000-0x40280640ff 64bit]
[    0.468483] pci 0000:00:1f.4: BAR 4 [io  0xefa0-0xefbf]
[    0.468714] pci 0000:00:1f.5: [8086:7723] type 00 class 0x0c8000 conventional PCI endpoint
[    0.468759] pci 0000:00:1f.5: BAR 0 [mem 0xfe010000-0xfe010fff]
[    0.469062] pci 0000:01:00.0: [14e4:16d8] type 00 class 0x020000 PCIe Endpoint
[    0.469091] pci 0000:01:00.0: BAR 0 [mem 0x4018300000-0x401830ffff 64bit pref]
[    0.469108] pci 0000:01:00.0: BAR 2 [mem 0x4018100000-0x40181fffff 64bit pref]
[    0.469126] pci 0000:01:00.0: BAR 4 [mem 0x4018320000-0x4018321fff 64bit pref]
[    0.469136] pci 0000:01:00.0: ROM [mem 0x81640000-0x8167ffff pref]
[    0.469148] pci 0000:01:00.0: Max Payload Size set to 256 (was 128, max 512)
[    0.469294] pci 0000:01:00.0: PME# supported from D0 D3hot D3cold
[    0.469439] pci 0000:01:00.0: 16.000 Gb/s available PCIe bandwidth, limited by 2.5 GT/s PCIe x8 link at 0000:00:01.0 (capable of 63.008 Gb/s with 8.0 GT/s PCIe x8 link)
[    0.469610] pci 0000:01:00.1: [14e4:16d8] type 00 class 0x020000 PCIe Endpoint
[    0.469641] pci 0000:01:00.1: BAR 0 [mem 0x4018310000-0x401831ffff 64bit pref]
[    0.469660] pci 0000:01:00.1: BAR 2 [mem 0x4018200000-0x40182fffff 64bit pref]
[    0.469679] pci 0000:01:00.1: BAR 4 [mem 0x4018322000-0x4018323fff 64bit pref]
[    0.469691] pci 0000:01:00.1: ROM [mem 0x81600000-0x8163ffff pref]
[    0.469703] pci 0000:01:00.1: Max Payload Size set to 256 (was 128, max 512)
[    0.469831] pci 0000:01:00.1: PME# supported from D0 D3hot D3cold
[    0.470026] pci 0000:00:01.0: PCI bridge to [bus 01]
[    0.470137] pci 0000:02:00.0: [1344:51c3] type 00 class 0x010802 PCIe Endpoint
[    0.470162] pci 0000:02:00.0: BAR 0 [mem 0x81540000-0x8157ffff 64bit]
[    0.470213] pci 0000:02:00.0: ROM [mem 0x81500000-0x8153ffff pref]
[    0.470299] pci 0000:02:00.0: PME# supported from D0 D1 D3hot
[    0.470451] pci 0000:00:06.0: PCI bridge to [bus 02]
[    0.470548] pci 0000:03:00.0: [1344:51c3] type 00 class 0x010802 PCIe Endpoint
[    0.470573] pci 0000:03:00.0: BAR 0 [mem 0x81440000-0x8147ffff 64bit]
[    0.470624] pci 0000:03:00.0: ROM [mem 0x81400000-0x8143ffff pref]
[    0.470709] pci 0000:03:00.0: PME# supported from D0 D1 D3hot
[    0.470862] pci 0000:00:06.2: PCI bridge to [bus 03]
[    0.470963] pci 0000:04:00.0: [14e4:165f] type 00 class 0x020000 PCIe Endpoint
[    0.470994] pci 0000:04:00.0: BAR 0 [mem 0x4018050000-0x401805ffff 64bit pref]
[    0.471013] pci 0000:04:00.0: BAR 2 [mem 0x4018040000-0x401804ffff 64bit pref]
[    0.471032] pci 0000:04:00.0: BAR 4 [mem 0x4018030000-0x401803ffff 64bit pref]
[    0.471045] pci 0000:04:00.0: ROM [mem 0x81340000-0x8137ffff pref]
[    0.471153] pci 0000:04:00.0: PME# supported from D0 D3hot D3cold
[    0.471435] pci 0000:04:00.1: [14e4:165f] type 00 class 0x020000 PCIe Endpoint
[    0.471465] pci 0000:04:00.1: BAR 0 [mem 0x4018020000-0x401802ffff 64bit pref]
[    0.471484] pci 0000:04:00.1: BAR 2 [mem 0x4018010000-0x401801ffff 64bit pref]
[    0.471503] pci 0000:04:00.1: BAR 4 [mem 0x4018000000-0x401800ffff 64bit pref]
[    0.471516] pci 0000:04:00.1: ROM [mem 0x81300000-0x8133ffff pref]
[    0.471625] pci 0000:04:00.1: PME# supported from D0 D3hot D3cold
[    0.471896] pci 0000:00:1c.0: PCI bridge to [bus 04]
[    0.471973] pci 0000:05:00.0: [1a03:1150] type 01 class 0x060400 PCIe to PCI/PCI-X bridge
[    0.472019] pci 0000:05:00.0: PCI bridge to [bus 06]
[    0.472028] pci 0000:05:00.0:   bridge window [io  0x3000-0x3fff]
[    0.472032] pci 0000:05:00.0:   bridge window [mem 0x80000000-0x812fffff]
[    0.472066] pci 0000:05:00.0: enabling Extended Tags
[    0.472154] pci 0000:05:00.0: supports D1 D2
[    0.472155] pci 0000:05:00.0: PME# supported from D0 D1 D2 D3hot D3cold
[    0.472312] pci 0000:00:1c.6: PCI bridge to [bus 05-06]
[    0.472376] pci_bus 0000:06: extended config space not accessible
[    0.472401] pci 0000:06:00.0: [1a03:2000] type 00 class 0x030000 conventional PCI endpoint
[    0.472427] pci 0000:06:00.0: BAR 0 [mem 0x80000000-0x80ffffff]
[    0.472442] pci 0000:06:00.0: BAR 1 [mem 0x81240000-0x8127ffff]
[    0.472456] pci 0000:06:00.0: BAR 2 [io  0x3000-0x307f]
[    0.472518] pci 0000:06:00.0: BAR 0: assigned to efifb
[    0.472562] pci 0000:06:00.0: supports D1 D2
[    0.472563] pci 0000:06:00.0: PME# supported from D0 D1 D2 D3hot D3cold
[    0.472675] pci 0000:05:00.0: PCI bridge to [bus 06]
[    0.478671] ACPI: PCI: Interrupt link LNKA configured for IRQ 0
[    0.478784] ACPI: PCI: Interrupt link LNKB configured for IRQ 1
[    0.478893] ACPI: PCI: Interrupt link LNKC configured for IRQ 0
[    0.479001] ACPI: PCI: Interrupt link LNKD configured for IRQ 0
[    0.479109] ACPI: PCI: Interrupt link LNKE configured for IRQ 0
[    0.479218] ACPI: PCI: Interrupt link LNKF configured for IRQ 0
[    0.479325] ACPI: PCI: Interrupt link LNKG configured for IRQ 0
[    0.479433] ACPI: PCI: Interrupt link LNKH configured for IRQ 0
[    0.487356] iommu: Default domain type: Passthrough (set via kernel command line)
[    0.487356] SCSI subsystem initialized
[    0.487356] ACPI: bus type USB registered
[    0.487356] usbcore: registered new interface driver usbfs
[    0.487356] usbcore: registered new interface driver hub
[    0.487356] usbcore: registered new device driver usb
[    0.487356] pps_core: LinuxPPS API ver. 1 registered
[    0.487356] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.487356] PTP clock support registered
[    0.487356] EDAC MC: Ver: 3.0.0
[    0.487356] Registered efivars operations
[    0.488148] NetLabel: Initializing
[    0.488149] NetLabel:  domain hash size = 128
[    0.488150] NetLabel:  protocols = UNLABELED CIPSOv4 CALIPSO
[    0.488168] NetLabel:  unlabeled traffic allowed by default
[    0.488169] PCI: Using ACPI for IRQ routing
[    0.510145] PCI: pci_cache_line_size set to 64 bytes
[    0.510207] pci 0000:00:1f.5: BAR 0 [mem 0xfe010000-0xfe010fff]: can't claim; no compatible bridge window
[    0.510228] pci 0000:01:00.0: BAR 0 [mem 0x4018300000-0x401830ffff 64bit pref]: can't claim; no compatible bridge window
[    0.510230] pci 0000:01:00.0: BAR 2 [mem 0x4018100000-0x40181fffff 64bit pref]: can't claim; no compatible bridge window
[    0.510231] pci 0000:01:00.0: BAR 4 [mem 0x4018320000-0x4018321fff 64bit pref]: can't claim; no compatible bridge window
[    0.510234] pci 0000:01:00.1: BAR 0 [mem 0x4018310000-0x401831ffff 64bit pref]: can't claim; no compatible bridge window
[    0.510235] pci 0000:01:00.1: BAR 2 [mem 0x4018200000-0x40182fffff 64bit pref]: can't claim; no compatible bridge window
[    0.510236] pci 0000:01:00.1: BAR 4 [mem 0x4018322000-0x4018323fff 64bit pref]: can't claim; no compatible bridge window
[    0.510291] e820: reserve RAM buffer [mem 0x58a10018-0x5bffffff]
[    0.510294] e820: reserve RAM buffer [mem 0x58b6d018-0x5bffffff]
[    0.510295] e820: reserve RAM buffer [mem 0x58b9f018-0x5bffffff]
[    0.510296] e820: reserve RAM buffer [mem 0x58bac018-0x5bffffff]
[    0.510297] e820: reserve RAM buffer [mem 0x612c4000-0x63ffffff]
[    0.510297] e820: reserve RAM buffer [mem 0x65bff000-0x67ffffff]
[    0.510298] e820: reserve RAM buffer [mem 0x6a000000-0x6bffffff]
[    0.510339] pci 0000:00:02.0: vgaarb: setting as boot VGA device
[    0.510339] pci 0000:00:02.0: vgaarb: bridge control possible
[    0.510339] pci 0000:00:02.0: vgaarb: VGA device added: decodes=io+mem,owns=io+mem,locks=none
[    0.510339] pci 0000:06:00.0: vgaarb: setting as boot VGA device (overriding previous)
[    0.510339] pci 0000:06:00.0: vgaarb: bridge control possible
[    0.510339] pci 0000:06:00.0: vgaarb: VGA device added: decodes=io+mem,owns=none,locks=none
[    0.510339] vgaarb: loaded
[    0.510339] clocksource: Switched to clocksource tsc-early
[    0.518659] VFS: Disk quotas dquot_6.6.0
[    0.518673] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.518726] pnp: PnP ACPI init
[    0.518801] pnp 00:00: [dma 0 disabled]
[    0.518969] system 00:01: [io  0x0680-0x069f] has been reserved
[    0.518971] system 00:01: [io  0x164e-0x164f] has been reserved
[    0.519104] system 00:02: [io  0x1854-0x1857] has been reserved
[    0.519187] system 00:03: [io  0x0cc0] has been reserved
[    0.519189] system 00:03: [io  0x0cc1] has been reserved
[    0.519216] system 00:04: [io  0x0c90-0x0c9f] has been reserved
[    0.519217] system 00:04: [io  0x0c00-0x0c0f] has been reserved
[    0.519219] system 00:04: [io  0x0cc2-0x0cc3] has been reserved
[    0.522493] system 00:05: [mem 0xfedc0000-0xfedc7fff] has been reserved
[    0.522495] system 00:05: [mem 0x00000000-0x00000fff] could not be reserved
[    0.522496] system 00:05: [mem 0x00000000-0x00000fff] could not be reserved
[    0.522498] system 00:05: [mem 0xc0000000-0xcfffffff] has been reserved
[    0.522499] system 00:05: [mem 0xfed20000-0xfed7ffff] could not be reserved
[    0.522501] system 00:05: [mem 0xfc800000-0xfc81ffff] could not be reserved
[    0.522502] system 00:05: [mem 0xfed45000-0xfed8ffff] could not be reserved
[    0.522503] system 00:05: [mem 0xfee00000-0xfeefffff] could not be reserved
[    0.523646] system 00:06: [io  0x2000-0x20fe] has been reserved
[    0.523936] system 00:07: [mem 0xfe02c008-0xfe02cfff] has been reserved
[    0.523938] system 00:07: [mem 0xfe02d000-0xfe02dfff] has been reserved
[    0.524274] pnp: PnP ACPI: found 8 devices
[    0.530048] clocksource: acpi_pm: mask: 0xffffff max_cycles: 0xffffff, max_idle_ns: 2085701024 ns
[    0.530131] NET: Registered PF_INET protocol family
[    0.530408] IP idents hash table entries: 262144 (order: 9, 2097152 bytes, linear)
[    0.533295] tcp_listen_portaddr_hash hash table entries: 32768 (order: 7, 524288 bytes, linear)
[    0.533364] Table-perturb hash table entries: 65536 (order: 6, 262144 bytes, linear)
[    0.533373] TCP established hash table entries: 524288 (order: 10, 4194304 bytes, linear)
[    0.533809] TCP bind hash table entries: 65536 (order: 8, 1048576 bytes, linear)
[    0.533942] TCP: Hash tables configured (established 524288 bind 65536)
[    0.534247] MPTCP token hash table entries: 65536 (order: 8, 1572864 bytes, linear)
[    0.534339] UDP hash table entries: 32768 (order: 8, 1048576 bytes, linear)
[    0.534472] UDP-Lite hash table entries: 32768 (order: 8, 1048576 bytes, linear)
[    0.534646] NET: Registered PF_UNIX/PF_LOCAL protocol family
[    0.534653] NET: Registered PF_XDP protocol family
[    0.534657] pci 0000:01:00.0: ROM [mem 0x81640000-0x8167ffff pref]: can't claim; no compatible bridge window
[    0.534659] pci 0000:01:00.1: ROM [mem 0x81600000-0x8163ffff pref]: can't claim; no compatible bridge window
[    0.534675] pci 0000:00:01.0: bridge window [mem 0x81700000-0x817fffff]: assigned
[    0.534677] pci 0000:00:01.0: bridge window [mem 0x4018100000-0x40183fffff 64bit pref]: assigned
[    0.534679] pci 0000:00:1f.5: BAR 0 [mem 0x81601000-0x81601fff]: assigned
[    0.534693] pci 0000:01:00.0: BAR 2 [mem 0x4018100000-0x40181fffff 64bit pref]: assigned
[    0.534708] pci 0000:01:00.1: BAR 2 [mem 0x4018200000-0x40182fffff 64bit pref]: assigned
[    0.534722] pci 0000:01:00.0: ROM [mem 0x81700000-0x8173ffff pref]: assigned
[    0.534724] pci 0000:01:00.1: ROM [mem 0x81740000-0x8177ffff pref]: assigned
[    0.534725] pci 0000:01:00.0: BAR 0 [mem 0x4018300000-0x401830ffff 64bit pref]: assigned
[    0.534739] pci 0000:01:00.1: BAR 0 [mem 0x4018310000-0x401831ffff 64bit pref]: assigned
[    0.534753] pci 0000:01:00.0: BAR 4 [mem 0x4018320000-0x4018321fff 64bit pref]: assigned
[    0.534767] pci 0000:01:00.1: BAR 4 [mem 0x4018322000-0x4018323fff 64bit pref]: assigned
[    0.534782] pci 0000:00:01.0: PCI bridge to [bus 01]
[    0.534787] pci 0000:00:01.0:   bridge window [mem 0x81700000-0x817fffff]
[    0.534790] pci 0000:00:01.0:   bridge window [mem 0x4018100000-0x40183fffff 64bit pref]
[    0.534797] pci 0000:00:06.0: PCI bridge to [bus 02]
[    0.534802] pci 0000:00:06.0:   bridge window [mem 0x81500000-0x815fffff]
[    0.534811] pci 0000:00:06.2: PCI bridge to [bus 03]
[    0.534816] pci 0000:00:06.2:   bridge window [mem 0x81400000-0x814fffff]
[    0.534825] pci 0000:00:1c.0: PCI bridge to [bus 04]
[    0.534830] pci 0000:00:1c.0:   bridge window [mem 0x81300000-0x813fffff]
[    0.534833] pci 0000:00:1c.0:   bridge window [mem 0x4018000000-0x40180fffff 64bit pref]
[    0.534839] pci 0000:05:00.0: PCI bridge to [bus 06]
[    0.534842] pci 0000:05:00.0:   bridge window [io  0x3000-0x3fff]
[    0.534848] pci 0000:05:00.0:   bridge window [mem 0x80000000-0x812fffff]
[    0.534858] pci 0000:00:1c.6: PCI bridge to [bus 05-06]
[    0.534860] pci 0000:00:1c.6:   bridge window [io  0x3000-0x3fff]
[    0.534865] pci 0000:00:1c.6:   bridge window [mem 0x80000000-0x812fffff]
[    0.534873] pci_bus 0000:00: resource 4 [io  0x0000-0x0cf7 window]
[    0.534875] pci_bus 0000:00: resource 5 [io  0x0d00-0xffff window]
[    0.534876] pci_bus 0000:00: resource 6 [mem 0x000a0000-0x000bffff window]
[    0.534877] pci_bus 0000:00: resource 7 [mem 0x80000000-0xbfffffff window]
[    0.534879] pci_bus 0000:00: resource 8 [mem 0x4000000000-0x3ffbfffffff window]
[    0.534880] pci_bus 0000:01: resource 1 [mem 0x81700000-0x817fffff]
[    0.534881] pci_bus 0000:01: resource 2 [mem 0x4018100000-0x40183fffff 64bit pref]
[    0.534882] pci_bus 0000:02: resource 1 [mem 0x81500000-0x815fffff]
[    0.534884] pci_bus 0000:03: resource 1 [mem 0x81400000-0x814fffff]
[    0.534885] pci_bus 0000:04: resource 1 [mem 0x81300000-0x813fffff]
[    0.534886] pci_bus 0000:04: resource 2 [mem 0x4018000000-0x40180fffff 64bit pref]
[    0.534887] pci_bus 0000:05: resource 0 [io  0x3000-0x3fff]
[    0.534888] pci_bus 0000:05: resource 1 [mem 0x80000000-0x812fffff]
[    0.534889] pci_bus 0000:06: resource 0 [io  0x3000-0x3fff]
[    0.534890] pci_bus 0000:06: resource 1 [mem 0x80000000-0x812fffff]
[    0.535388] PCI: CLS 64 bytes, default 64
[    0.535409] DMAR: No RMRR found
[    0.535410] DMAR: No ATSR found
[    0.535411] DMAR: IOMMU feature sc_support inconsistent
[    0.535413] DMAR: dmar0: Using Queued invalidation
[    0.535418] DMAR: dmar1: Using Queued invalidation
[    0.535453] Trying to unpack rootfs image as initramfs...
[    0.535848] pci 0000:00:02.0: Adding to iommu group 0
[    0.535884] pci 0000:00:00.0: Adding to iommu group 1
[    0.535903] pci 0000:00:01.0: Adding to iommu group 2
[    0.535919] pci 0000:00:06.0: Adding to iommu group 3
[    0.535936] pci 0000:00:06.2: Adding to iommu group 4
[    0.535949] pci 0000:00:08.0: Adding to iommu group 5
[    0.535962] pci 0000:00:0a.0: Adding to iommu group 6
[    0.535976] pci 0000:00:0b.0: Adding to iommu group 7
[    0.535995] pci 0000:00:0d.0: Adding to iommu group 8
[    0.536021] pci 0000:00:14.0: Adding to iommu group 9
[    0.536035] pci 0000:00:14.2: Adding to iommu group 9
[    0.536058] pci 0000:00:16.0: Adding to iommu group 10
[    0.536073] pci 0000:00:16.3: Adding to iommu group 10
[    0.536088] pci 0000:00:1c.0: Adding to iommu group 11
[    0.536103] pci 0000:00:1c.6: Adding to iommu group 12
[    0.536132] pci 0000:00:1f.0: Adding to iommu group 13
[    0.536147] pci 0000:00:1f.4: Adding to iommu group 13
[    0.536161] pci 0000:00:1f.5: Adding to iommu group 13
[    0.536186] pci 0000:01:00.0: Adding to iommu group 14
[    0.536202] pci 0000:01:00.1: Adding to iommu group 14
[    0.536220] pci 0000:02:00.0: Adding to iommu group 15
[    0.536238] pci 0000:03:00.0: Adding to iommu group 16
[    0.536266] pci 0000:04:00.0: Adding to iommu group 17
[    0.536284] pci 0000:04:00.1: Adding to iommu group 17
[    0.536300] pci 0000:05:00.0: Adding to iommu group 18
[    0.536308] pci 0000:06:00.0: Adding to iommu group 18
[    0.536632] DMAR: Intel(R) Virtualization Technology for Directed I/O
[    0.536633] PCI-DMA: Using software bounce buffering for IO (SWIOTLB)
[    0.536634] software IO TLB: mapped [mem 0x00000000528dd000-0x00000000568dd000] (64MB)
[    0.536645] ACPI: bus type thunderbolt registered
[    0.536706] clocksource: tsc: mask: 0xffffffffffffffff max_cycles: 0x6a464ae9873, max_idle_ns: 881590529744 ns
[    0.536746] clocksource: Switched to clocksource tsc
[    0.536761] platform rtc_cmos: registered platform RTC device (no PNP device found)
[    0.539093] Initialise system trusted keyrings
[    0.539103] Key type blacklist registered
[    0.539145] workingset: timestamp_bits=36 max_order=24 bucket_order=0
[    0.539158] zbud: loaded
[    0.539471] integrity: Platform Keyring initialized
[    0.539475] integrity: Machine keyring initialized
[    0.549797] NET: Registered PF_ALG protocol family
[    0.549799] xor: automatically using best checksumming function   avx       
[    0.549801] Key type asymmetric registered
[    0.549803] Asymmetric key parser 'x509' registered
[    0.549804] Running certificate verification selftests
[    0.551228] Loaded X.509 cert 'Certificate verification self-testing key: f58703bb33ce1b73ee02eccdee5b8817518fe3db'
[    0.551759] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 246)
[    0.551808] io scheduler mq-deadline registered
[    0.551809] io scheduler kyber registered
[    0.551817] io scheduler bfq registered
[    0.553923] atomic64_test: passed for x86-64 platform with CX8 and with SSE
[    0.554289] pcieport 0000:00:01.0: PME: Signaling with IRQ 122
[    0.554349] pcieport 0000:00:01.0: AER: enabled with IRQ 122
[    0.554577] pcieport 0000:00:06.0: PME: Signaling with IRQ 123
[    0.554631] pcieport 0000:00:06.0: AER: enabled with IRQ 123
[    0.554857] pcieport 0000:00:06.2: PME: Signaling with IRQ 124
[    0.554907] pcieport 0000:00:06.2: AER: enabled with IRQ 124
[    0.555117] pcieport 0000:00:1c.0: PME: Signaling with IRQ 125
[    0.555163] pcieport 0000:00:1c.0: AER: enabled with IRQ 125
[    0.555354] pcieport 0000:00:1c.6: PME: Signaling with IRQ 126
[    0.555401] pcieport 0000:00:1c.6: AER: enabled with IRQ 126
[    0.555510] shpchp: Standard Hot Plug PCI Controller Driver version: 0.4
[    0.555693] Monitor-Mwait will be used to enter C-1 state
[    0.555706] Monitor-Mwait will be used to enter C-2 state
[    0.555720] Monitor-Mwait will be used to enter C-3 state
[    0.555725] ACPI: \_SB_.PR00: Found 3 idle states
[    0.556767] input: Sleep Button as /devices/LNXSYSTM:00/LNXSYBUS:00/PNP0C0E:00/input/input0
[    0.556811] ACPI: button: Sleep Button [SLPB]
[    0.556838] input: Power Button as /devices/LNXSYSTM:00/LNXSYBUS:00/PNP0C0C:00/input/input1
[    0.556851] ACPI: button: Power Button [PWRB]
[    0.556877] input: Power Button as /devices/LNXSYSTM:00/LNXPWRBN:00/input/input2
[    0.556995] ACPI: button: Power Button [PWRF]
[    0.563940] Serial: 8250/16550 driver, 4 ports, IRQ sharing enabled
[    0.564070] 00:00: ttyS0 at I/O 0x3f8 (irq = 4, base_baud = 115200) is a 16550A
[    0.564470] serial 0000:00:16.3: enabling device (0000 -> 0003)
[    0.564757] 0000:00:16.3: ttyS1 at I/O 0x4020 (irq = 19, base_baud = 115200) is a 16550A
[    0.564967] hpet_acpi_add: no address or irqs in _CRS
[    0.565018] Non-volatile memory driver v1.3
[    0.577816] tpm_tis MSFT0101:00: 2.0 TPM (device-id 0xFC, rev-id 1)
[    0.595326] rdac: device handler registered
[    0.595453] hp_sw: device handler registered
[    0.595454] emc: device handler registered
[    0.595497] alua: device handler registered
[    0.595711] xhci_hcd 0000:00:0d.0: xHCI Host Controller
[    0.595810] xhci_hcd 0000:00:0d.0: new USB bus registered, assigned bus number 1
[    0.596892] xhci_hcd 0000:00:0d.0: hcc params 0x20007fc1 hci version 0x120 quirks 0x0000000200009810
[    0.597195] xhci_hcd 0000:00:0d.0: xHCI Host Controller
[    0.597221] xhci_hcd 0000:00:0d.0: new USB bus registered, assigned bus number 2
[    0.597223] xhci_hcd 0000:00:0d.0: Host supports USB 3.2 Enhanced SuperSpeed
[    0.597263] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 5.14
[    0.597266] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    0.597268] usb usb1: Product: xHCI Host Controller
[    0.597269] usb usb1: Manufacturer: Linux 5.14.0-529.el9.x86_64 xhci-hcd
[    0.597271] usb usb1: SerialNumber: 0000:00:0d.0
[    0.597356] hub 1-0:1.0: USB hub found
[    0.597365] hub 1-0:1.0: 1 port detected
[    0.597561] usb usb2: New USB device found, idVendor=1d6b, idProduct=0003, bcdDevice= 5.14
[    0.597563] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    0.597564] usb usb2: Product: xHCI Host Controller
[    0.597565] usb usb2: Manufacturer: Linux 5.14.0-529.el9.x86_64 xhci-hcd
[    0.597566] usb usb2: SerialNumber: 0000:00:0d.0
[    0.597630] hub 2-0:1.0: USB hub found
[    0.597640] hub 2-0:1.0: 4 ports detected
[    0.599244] xhci_hcd 0000:00:14.0: xHCI Host Controller
[    0.599270] xhci_hcd 0000:00:14.0: new USB bus registered, assigned bus number 3
[    0.600348] xhci_hcd 0000:00:14.0: hcc params 0x20007fc1 hci version 0x120 quirks 0x0000000200009810
[    0.600604] xhci_hcd 0000:00:14.0: xHCI Host Controller
[    0.600632] xhci_hcd 0000:00:14.0: new USB bus registered, assigned bus number 4
[    0.600634] xhci_hcd 0000:00:14.0: Host supports USB 3.2 Enhanced SuperSpeed
[    0.600657] usb usb3: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 5.14
[    0.600659] usb usb3: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    0.600660] usb usb3: Product: xHCI Host Controller
[    0.600661] usb usb3: Manufacturer: Linux 5.14.0-529.el9.x86_64 xhci-hcd
[    0.600662] usb usb3: SerialNumber: 0000:00:14.0
[    0.600883] hub 3-0:1.0: USB hub found
[    0.600896] hub 3-0:1.0: 12 ports detected
[    0.602301] usb usb4: New USB device found, idVendor=1d6b, idProduct=0003, bcdDevice= 5.14
[    0.602303] usb usb4: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    0.602304] usb usb4: Product: xHCI Host Controller
[    0.602305] usb usb4: Manufacturer: Linux 5.14.0-529.el9.x86_64 xhci-hcd
[    0.602306] usb usb4: SerialNumber: 0000:00:14.0
[    0.602367] hub 4-0:1.0: USB hub found
[    0.602374] hub 4-0:1.0: 2 ports detected
[    0.602698] usbcore: registered new interface driver usbserial_generic
[    0.602703] usbserial: USB Serial support registered for generic
[    0.602735] i8042: PNP: No PS/2 controller found.
[    0.602760] mousedev: PS/2 mouse device common for all mice
[    0.602860] rtc_cmos rtc_cmos: RTC can wake from S4
[    0.603723] rtc_cmos rtc_cmos: registered as rtc0
[    0.603904] rtc_cmos rtc_cmos: setting system clock to 2024-11-29T08:50:34 UTC (1732870234)
[    0.603931] rtc_cmos rtc_cmos: alarms up to one month, y3k, 114 bytes nvram
[    0.605047] intel_pstate: Intel P-state driver initializing
[    0.607461] Hybrid CPU capacity scaling enabled
[    0.608282] intel_pstate: HWP enabled
[    0.608503] efifb: probing for efifb
[    0.608517] efifb: framebuffer at 0x80000000, using 3072k, total 3072k
[    0.608519] efifb: mode is 1024x768x32, linelength=4096, pages=1
[    0.608521] efifb: scrolling: redraw
[    0.608521] efifb: Truecolor: size=8:8:8:8, shift=24:16:8:0
[    0.608606] Console: switching to colour frame buffer device 128x48
[    0.616942] fb0: EFI VGA frame buffer device
[    0.616947] EFI Variables Facility v0.08 2004-May-17
[    0.625423] hid: raw HID events driver (C) Jiri Kosina
[    0.625467] usbcore: registered new interface driver usbhid
[    0.625469] usbhid: USB HID core driver
[    0.625495] drop_monitor: Initializing network drop monitor service
[    0.639111] Initializing XFRM netlink socket
[    0.639140] NET: Registered PF_INET6 protocol family
[    0.905624] usb 3-1: new full-speed USB device number 2 using xhci_hcd
[    1.107955] usb 3-1: not running at top speed; connect to a high speed hub
[    1.121204] usb 3-1: New USB device found, idVendor=17ef, idProduct=7217, bcdDevice=10.04
[    1.121212] usb 3-1: New USB device strings: Mfr=1, Product=2, SerialNumber=3
[    1.121214] usb 3-1: Product: Lenovo USB-C to VGA Adapter   
[    1.121216] usb 3-1: Manufacturer: VIA Technologies Inc.         
[    1.121218] usb 3-1: SerialNumber: 0000000000000001
[    1.244629] usb 3-5: new low-speed USB device number 3 using xhci_hcd
[    1.376435] usb 3-5: New USB device found, idVendor=04b3, idProduct=3025, bcdDevice= 1.02
[    1.376443] usb 3-5: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[    1.376446] usb 3-5: Product: USB NetVista Full Width Keyboard
[    1.376448] usb 3-5: Manufacturer: CHICONY
[    1.380269] input: CHICONY USB NetVista Full Width Keyboard as /devices/pci0000:00/0000:00:14.0/usb3/3-5/3-5:1.0/0003:04B3:3025.0001/input/input3
[    1.432054] hid-generic 0003:04B3:3025.0001: input,hidraw0: USB HID v1.10 Keyboard [CHICONY USB NetVista Full Width Keyboard] on usb-0000:00:14.0-5/input0
[    1.518935] Freeing initrd memory: 75612K
[    1.527345] Segment Routing with IPv6
[    1.527377] NET: Registered PF_PACKET protocol family
[    1.527503] mpls_gso: MPLS GSO support
[    1.531044] ENERGY_PERF_BIAS: Set to 'normal', was 'performance'
[    1.532324] microcode: Current revision: 0x00000109
[    1.533600] IPI shorthand broadcast: enabled
[    1.533612] AVX2 version of gcm_enc/dec engaged.
[    1.534824] AES CTR mode by8 optimization enabled
[    1.534888] sched_clock: Marking stable (1528001722, 6617810)->(1566787364, -32167832)
[    1.535304] registered taskstats version 1
[    1.537163] Loading compiled-in X.509 certificates
[    1.538485] Loaded X.509 cert 'Red Hat Enterprise Linux kernel signing key: 8929d135ae0fa6510b40ccdbd3dbbf0b2663dd67'
[    1.538831] Loaded X.509 cert 'Red Hat Enterprise Linux Driver Update Program (key 3): bf57f3e87362bc7229d9f465321773dfd1f77a80'
[    1.539151] Loaded X.509 cert 'Red Hat Enterprise Linux kpatch signing key: 4d38fd864ebe18c5f0b72e3852e2014c3a676fc8'
[    1.539333] Loaded X.509 cert 'RH-IMA-CA: Red Hat IMA CA: fb31825dd0e073685b264e3038963673f753959a'
[    1.539341] Loaded X.509 cert 'Nvidia GPU OOT signing 001: 55e1cef88193e60419f0b0ec379c49f77545acf0'
[    1.541308] Demotion targets for Node 0: null
[    1.541311] page_owner is disabled
[    1.541788] Key type .fscrypt registered
[    1.541789] Key type fscrypt-provisioning registered
[    1.541822] Key type big_key registered
[    1.544935] Key type trusted registered
[    1.546645] usb 3-7: new low-speed USB device number 4 using xhci_hcd
[    1.548307] Key type encrypted registered
[    1.551651] integrity: Loading X.509 certificate: UEFI:MokListRT (MOKvar table)
[    1.551828] integrity: Loading X.509 certificate: UEFI:MokListRT (MOKvar table)
[    1.551979] integrity: Loaded X.509 cert 'Red Hat Secure Boot CA 5: cc6fa5e72868ba494e939bbd680b9144769a9f8f'
[    1.551980] integrity: Loading X.509 certificate: UEFI:MokListRT (MOKvar table)
[    1.552516] integrity: Loading X.509 certificate: UEFI:MokListRT (MOKvar table)
[    1.553088] integrity: Loaded X.509 cert 'Red Hat Secure Boot CA 8: e1c6c580aa1e21d585aad9bf20f3929e5ec1f08b'
[    1.553092] Loading compiled-in module X.509 certificates
[    1.553432] Loaded X.509 cert 'Red Hat Enterprise Linux kernel signing key: 8929d135ae0fa6510b40ccdbd3dbbf0b2663dd67'
[    1.553434] ima: Allocated hash algorithm: sha256
[    1.586177] ima: No architecture policies found
[    1.586193] evm: Initialising EVM extended attributes:
[    1.586194] evm: security.selinux
[    1.586195] evm: security.SMACK64 (disabled)
[    1.586196] evm: security.SMACK64EXEC (disabled)
[    1.586197] evm: security.SMACK64TRANSMUTE (disabled)
[    1.586197] evm: security.SMACK64MMAP (disabled)
[    1.586198] evm: security.apparmor (disabled)
[    1.586199] evm: security.ima
[    1.586199] evm: security.capability
[    1.586200] evm: HMAC attrs: 0x1
[    1.676871] usb 3-7: New USB device found, idVendor=046d, idProduct=c077, bcdDevice=72.00
[    1.676879] usb 3-7: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[    1.676882] usb 3-7: Product: USB Optical Mouse
[    1.676884] usb 3-7: Manufacturer: Logitech
[    1.680116] input: Logitech USB Optical Mouse as /devices/pci0000:00/0000:00:14.0/usb3/3-7/3-7:1.0/0003:046D:C077.0002/input/input4
[    1.680565] hid-generic 0003:046D:C077.0002: input,hidraw1: USB HID v1.11 Mouse [Logitech USB Optical Mouse] on usb-0000:00:14.0-7/input0
[    1.794633] usb 3-9: new high-speed USB device number 5 using xhci_hcd
[    1.813635] PM: hibernation: Checking hibernation image partition /dev/mapper/rhel-swap
[    1.813668] clk: Disabling unused clocks
[    1.819854] Freeing unused decrypted memory: 2028K
[    1.820693] Freeing unused kernel image (initmem) memory: 4020K
[    1.820694] Write protecting the kernel read-only data: 30720k
[    1.821648] Freeing unused kernel image (rodata/data gap) memory: 1152K
[    1.830545] x86/mm: Checked W+X mappings: passed, no W+X pages found.
[    1.830552] Run /init as init process
[    1.830553]   with arguments:
[    1.830554]     /init
[    1.830555]     rhgb
[    1.830556]   with environment:
[    1.830556]     HOME=/
[    1.830557]     TERM=linux
[    1.830558]     BOOT_IMAGE=(hd4,gpt2)/vmlinuz-5.14.0-529.el9.x86_64
[    1.878002] systemd[1]: systemd 252-48.el9 running in system mode (+PAM +AUDIT +SELINUX -APPARMOR +IMA +SMACK +SECCOMP +GCRYPT +GNUTLS +OPENSSL +ACL +BLKID +CURL +ELFUTILS +FIDO2 +IDN2 -IDN -IPTC +KMOD +LIBCRYPTSETUP +LIBFDISK +PCRE2 -PWQUALITY +P11KIT -QRENCODE +TPM2 +BZIP2 +LZ4 +XZ +ZLIB +ZSTD -BPF_FRAMEWORK +XKBCOMMON +UTMP +SYSVINIT default-hierarchy=unified)
[    1.878177] systemd[1]: Detected architecture x86-64.
[    1.878181] systemd[1]: Running in initrd.
[    1.878289] systemd[1]: No hostname configured, using default hostname.
[    1.878338] systemd[1]: Hostname set to <localhost>.
[    1.922015] usb 3-9: New USB device found, idVendor=1d6b, idProduct=0107, bcdDevice= 1.00
[    1.922026] usb 3-9: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    1.922030] usb 3-9: Product: USB Virtual Hub
[    1.922032] usb 3-9: Manufacturer: Aspeed
[    1.922034] usb 3-9: SerialNumber: 00000000
[    1.923392] hub 3-9:1.0: USB hub found
[    1.923549] hub 3-9:1.0: 7 ports detected
[    1.952953] systemd[1]: Queued start job for default target Initrd Default Target.
[    1.965290] systemd[1]: Created slice Slice /system/rdma-load-modules.
[    1.965612] systemd[1]: Created slice Slice /system/systemd-hibernate-resume.
[    1.965675] systemd[1]: Reached target Initrd /usr File System.
[    1.965707] systemd[1]: Reached target Slice Units.
[    1.965727] systemd[1]: Reached target Swaps.
[    1.965740] systemd[1]: Reached target Timer Units.
[    1.965849] systemd[1]: Listening on D-Bus System Message Bus Socket.
[    1.965946] systemd[1]: Listening on Journal Socket (/dev/log).
[    1.966045] systemd[1]: Listening on Journal Socket.
[    1.966148] systemd[1]: Listening on udev Control Socket.
[    1.966220] systemd[1]: Listening on udev Kernel Socket.
[    1.966235] systemd[1]: Reached target Socket Units.
[    1.967141] systemd[1]: Starting Create List of Static Device Nodes...
[    1.968088] systemd[1]: Starting Load RDMA modules from /etc/rdma/modules/infiniband.conf...
[    1.968979] systemd[1]: Starting Load RDMA modules from /etc/rdma/modules/rdma.conf...
[    1.969904] systemd[1]: Starting Load RDMA modules from /etc/rdma/modules/roce.conf...
[    1.971969] systemd[1]: Starting Journal Service...
[    1.972915] systemd[1]: Starting Load Kernel Modules...
[    1.973793] systemd[1]: Starting Create System Users...
[    1.974582] systemd[1]: Starting Setup Virtual Console...
[    1.975874] systemd[1]: Finished Create List of Static Device Nodes.
[    1.976167] systemd[1]: Finished Load RDMA modules from /etc/rdma/modules/roce.conf.
[    1.981611] systemd[1]: Finished Create System Users.
[    1.982607] systemd[1]: Starting Create Static Device Nodes in /dev...
[    1.996399] systemd[1]: Finished Create Static Device Nodes in /dev.
[    1.996795] Loading iSCSI transport class v2.0-870.
[    2.010555] fuse: init (API version 7.37)
[    2.014547] systemd[1]: Finished Load Kernel Modules.
[    2.043891] systemd[1]: Starting Apply Kernel Variables...
[    2.044090] systemd[1]: Started Journal Service.
[    2.120350] iscsi: registered transport (iser)
[    2.177088] Rounding down aligned max_sectors from 4294967295 to 4294967288
[    2.177141] db_root: cannot open: /etc/target
[    2.190340] device-mapper: core: CONFIG_IMA_DISABLE_HTABLE is disabled. Duplicate IMA measurements will not be recorded in the IMA log.
[    2.190371] device-mapper: uevent: version 1.0.3
[    2.190548] device-mapper: ioctl: 4.48.0-ioctl (2023-03-01) initialised: dm-devel@lists.linux.dev
[    2.194630] usb 3-9.1: new high-speed USB device number 6 using xhci_hcd
[    2.271356] usb 3-9.1: New USB device found, idVendor=17ef, idProduct=b000, bcdDevice= 0.00
[    2.271364] usb 3-9.1: New USB device strings: Mfr=4, Product=5, SerialNumber=6
[    2.271367] usb 3-9.1: Product: Keyboard/Mouse Function
[    2.271369] usb 3-9.1: Manufacturer: Avocent
[    2.271371] usb 3-9.1: SerialNumber: 20221116
[    2.280151] input: Avocent Keyboard/Mouse Function as /devices/pci0000:00/0000:00:14.0/usb3/3-9/3-9.1/3-9.1:1.0/0003:17EF:B000.0003/input/input5
[    2.332911] hid-generic 0003:17EF:B000.0003: input,hidraw2: USB HID v1.00 Keyboard [Avocent Keyboard/Mouse Function] on usb-0000:00:14.0-9.1/input0
[    2.333485] input: Avocent Keyboard/Mouse Function as /devices/pci0000:00/0000:00:14.0/usb3/3-9/3-9.1/3-9.1:1.1/0003:17EF:B000.0004/input/input6
[    2.333646] hid-generic 0003:17EF:B000.0004: input,hidraw3: USB HID v1.00 Mouse [Avocent Keyboard/Mouse Function] on usb-0000:00:14.0-9.1/input1
[    2.334460] input: Avocent Keyboard/Mouse Function as /devices/pci0000:00/0000:00:14.0/usb3/3-9/3-9.1/3-9.1:1.2/0003:17EF:B000.0005/input/input7
[    2.334552] hid-generic 0003:17EF:B000.0005: input,hidraw4: USB HID v1.00 Mouse [Avocent Keyboard/Mouse Function] on usb-0000:00:14.0-9.1/input2
[    2.345699] RPC: Registered named UNIX socket transport module.
[    2.345703] RPC: Registered udp transport module.
[    2.345704] RPC: Registered tcp transport module.
[    2.345705] RPC: Registered tcp-with-tls transport module.
[    2.345706] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    2.347363] acpi PNP0C14:01: duplicate WMI GUID 05901221-D566-11D1-B2F0-00A0C9062910 (first instance was on PNP0C14:00)
[    2.382082] RPC: Registered rdma transport module.
[    2.382088] RPC: Registered rdma backchannel transport module.
[    2.400640] usb 3-9.6: new high-speed USB device number 7 using xhci_hcd
[    2.402659] bnxt_en 0000:01:00.0: enabling device (0000 -> 0002)
[    2.408074] tg3 0000:04:00.0 eth0: Tigon3 [partno(N/A) rev 5720000] (PCI Express) MAC address 8c:3b:4a:9a:b5:7c
[    2.408084] tg3 0000:04:00.0 eth0: attached PHY is 5720C (10/100/1000Base-T Ethernet) (WireSpeed[1], EEE[1])
[    2.408087] tg3 0000:04:00.0 eth0: RXcsums[1] LinkChgREG[0] MIirq[0] ASF[1] TSOcap[1]
[    2.408090] tg3 0000:04:00.0 eth0: dma_rwctrl[00000001] dma_mask[64-bit]
[    2.431681] tg3 0000:04:00.1 eth1: Tigon3 [partno(N/A) rev 5720000] (PCI Express) MAC address 8c:3b:4a:9a:b5:7d
[    2.431691] tg3 0000:04:00.1 eth1: attached PHY is 5720C (10/100/1000Base-T Ethernet) (WireSpeed[1], EEE[1])
[    2.431694] tg3 0000:04:00.1 eth1: RXcsums[1] LinkChgREG[0] MIirq[0] ASF[1] TSOcap[1]
[    2.431696] tg3 0000:04:00.1 eth1: dma_rwctrl[00000001] dma_mask[64-bit]
[    2.433445] tg3 0000:04:00.0 eno1: renamed from eth0
[    2.452838] nvme nvme1: pci function 0000:03:00.0
[    2.452845] nvme nvme0: pci function 0000:02:00.0
[    2.452927] ACPI: bus type drm_connector registered
[    2.461487] nvme nvme0: 14/0/0 default/read/poll queues
[    2.463523] nvme nvme1: 14/0/0 default/read/poll queues
[    2.463813] tg3 0000:04:00.1 eno2: renamed from eth1
[    2.464685]  nvme0n1: p1 p2 p3
[    2.466977]  nvme1n1:
[    2.477399] usb 3-9.6: New USB device found, idVendor=04b3, idProduct=4010, bcdDevice= 5.04
[    2.477407] usb 3-9.6: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[    2.477410] usb 3-9.6: Product: XClarity Controller
[    2.477412] usb 3-9.6: Manufacturer: IBM
[    2.628752] bnxt_en 0000:01:00.0 (unnamed net_device) (uninitialized): Device requests max timeout of 100 seconds, may trigger hung task watchdog
[    2.766626] bnxt_en 0000:01:00.0 eth0: Broadcom BCM57416 NetXtreme-E 10GBase-T Ethernet found at mem 4018300000, node addr bc:97:e1:c9:dd:60
[    2.766644] bnxt_en 0000:01:00.0: 16.000 Gb/s available PCIe bandwidth, limited by 2.5 GT/s PCIe x8 link at 0000:00:01.0 (capable of 63.008 Gb/s with 8.0 GT/s PCIe x8 link)
[    2.766860] bnxt_en 0000:01:00.1: enabling device (0000 -> 0002)
[    2.767129] bnxt_en 0000:01:00.1 (unnamed net_device) (uninitialized): Device requests max timeout of 100 seconds, may trigger hung task watchdog
[    2.793745] bnxt_en 0000:01:00.1 eth1: Broadcom BCM57416 NetXtreme-E 10GBase-T Ethernet found at mem 4018310000, node addr bc:97:e1:c9:dd:61
[    2.793755] bnxt_en 0000:01:00.1: 16.000 Gb/s available PCIe bandwidth, limited by 2.5 GT/s PCIe x8 link at 0000:00:01.0 (capable of 63.008 Gb/s with 8.0 GT/s PCIe x8 link)
[    3.016013] bnxt_en 0000:01:00.1 ens4f1np1: renamed from eth1
[    3.220772] bnxt_en 0000:01:00.0 ens4f0np0: renamed from eth0
[    3.370163] bnxt_re: Broadcom NetXtreme-C/E RoCE Driver
[    3.648647] PM: hibernation: Configured hibernation resume from disk to 265289729
[    3.648655] PM: hibernation: Hibernation image partition 253:1 present
[    3.648658] PM: hibernation: Looking for hibernation image.
[    3.648768] PM: Image not found (code -22)
[    3.648770] PM: hibernation: Hibernation image not present or could not be loaded.
[    4.468053] SGI XFS with ACLs, security attributes, scrub, quota, no debug enabled
[    4.471898] XFS (dm-0): Mounting V5 Filesystem 5f49aa9c-4a72-48e3-a32d-dd2e67484182
[    4.480421] XFS (dm-0): Ending clean mount
[    4.629692] systemd-journald[346]: Received SIGTERM from PID 1 (systemd).
[    4.697868] audit: type=1404 audit(1732870238.592:2): enforcing=1 old_enforcing=0 auid=4294967295 ses=4294967295 enabled=1 old-enabled=1 lsm=selinux res=1
[    4.741993] SELinux:  policy capability network_peer_controls=1
[    4.741998] SELinux:  policy capability open_perms=1
[    4.741999] SELinux:  policy capability extended_socket_class=1
[    4.742001] SELinux:  policy capability always_check_network=0
[    4.742001] SELinux:  policy capability cgroup_seclabel=1
[    4.742002] SELinux:  policy capability nnp_nosuid_transition=1
[    4.742003] SELinux:  policy capability genfs_seclabel_symlinks=1
[    4.797594] audit: type=1403 audit(1732870238.691:3): auid=4294967295 ses=4294967295 lsm=selinux res=1
[    4.799572] systemd[1]: Successfully loaded SELinux policy in 102.253ms.
[    4.844041] systemd[1]: Relabelled /dev, /dev/shm, /run, /sys/fs/cgroup in 34.902ms.
[    4.850201] systemd[1]: systemd 252-48.el9 running in system mode (+PAM +AUDIT +SELINUX -APPARMOR +IMA +SMACK +SECCOMP +GCRYPT +GNUTLS +OPENSSL +ACL +BLKID +CURL +ELFUTILS +FIDO2 +IDN2 -IDN -IPTC +KMOD +LIBCRYPTSETUP +LIBFDISK +PCRE2 -PWQUALITY +P11KIT -QRENCODE +TPM2 +BZIP2 +LZ4 +XZ +ZLIB +ZSTD -BPF_FRAMEWORK +XKBCOMMON +UTMP +SYSVINIT default-hierarchy=unified)
[    4.850372] systemd[1]: Detected architecture x86-64.
[    4.887651] systemd-rc-local-generator[740]: /etc/rc.d/rc.local is not marked executable, skipping.
[    5.142929] systemd[1]: initrd-switch-root.service: Deactivated successfully.
[    5.143069] systemd[1]: Stopped Switch Root.
[    5.143805] systemd[1]: systemd-journald.service: Scheduled restart job, restart counter is at 1.
[    5.144288] systemd[1]: Created slice Virtual Machine and Container Slice.
[    5.144850] systemd[1]: Created slice Slice /system/getty.
[    5.145357] systemd[1]: Created slice Slice /system/modprobe.
[    5.145844] systemd[1]: Created slice Slice /system/sshd-keygen.
[    5.146319] systemd[1]: Created slice Slice /system/systemd-fsck.
[    5.146751] systemd[1]: Created slice User and Session Slice.
[    5.146803] systemd[1]: Dispatch Password Requests to Console Directory Watch was skipped because of an unmet condition check (ConditionPathExists=!/run/plymouth/pid).
[    5.146947] systemd[1]: Started Forward Password Requests to Wall Directory Watch.
[    5.147404] systemd[1]: Set up automount Arbitrary Executable File Formats File System Automount Point.
[    5.147478] systemd[1]: Reached target Local Encrypted Volumes.
[    5.147521] systemd[1]: Reached target Login Prompts.
[    5.147568] systemd[1]: Stopped target Switch Root.
[    5.147609] systemd[1]: Stopped target Initrd File Systems.
[    5.147704] systemd[1]: Stopped target Initrd Root File System.
[    5.147742] systemd[1]: Reached target Local Integrity Protected Volumes.
[    5.147825] systemd[1]: Reached target Slice Units.
[    5.147877] systemd[1]: Reached target Local Verity Protected Volumes.
[    5.148373] systemd[1]: Listening on Device-mapper event daemon FIFOs.
[    5.149582] systemd[1]: Listening on LVM2 poll daemon socket.
[    5.149727] systemd[1]: multipathd control socket was skipped because of an unmet condition check (ConditionPathExists=/etc/multipath.conf).
[    5.165875] systemd[1]: Listening on RPCbind Server Activation Socket.
[    5.165979] systemd[1]: Reached target RPC Port Mapper.
[    5.167370] systemd[1]: Listening on Process Core Dump Socket.
[    5.167484] systemd[1]: Listening on initctl Compatibility Named Pipe.
[    5.168407] systemd[1]: Listening on udev Control Socket.
[    5.168662] systemd[1]: Listening on udev Kernel Socket.
[    5.169788] systemd[1]: Activating swap /dev/mapper/rhel-swap...
[    5.171036] systemd[1]: Mounting Huge Pages File System...
[    5.172224] systemd[1]: Mounting POSIX Message Queue File System...
[    5.173274] systemd[1]: Mounting Kernel Debug File System...
[    5.174337] systemd[1]: Mounting Kernel Trace File System...
[    5.174484] systemd[1]: Kernel Module supporting RPCSEC_GSS was skipped because of an unmet condition check (ConditionPathExists=/etc/krb5.keytab).
[    5.174799] systemd[1]: iscsi-starter.service was skipped because of an unmet condition check (ConditionDirectoryNotEmpty=/var/lib/iscsi/nodes).
[    5.176465] systemd[1]: Starting Create List of Static Device Nodes...
[    5.177625] systemd[1]: Starting Monitoring of LVM2 mirrors, snapshots etc. using dmeventd or progress polling...
[    5.178732] systemd[1]: Starting Load Kernel Module configfs...
[    5.178927] Adding 31743996k swap on /dev/mapper/rhel-swap.  Priority:-2 extents:1 across:31743996k SS
[    5.179762] systemd[1]: Starting Load Kernel Module drm...
[    5.180742] systemd[1]: Starting Load Kernel Module efi_pstore...
[    5.181759] systemd[1]: Starting Load Kernel Module fuse...
[    5.183024] systemd[1]: Starting Read and set NIS domainname from /etc/sysconfig/network...
[    5.183131] systemd[1]: plymouth-switch-root.service: Deactivated successfully.
[    5.183179] systemd[1]: Stopped Plymouth switch root service.
[    5.183435] systemd[1]: systemd-fsck-root.service: Deactivated successfully.
[    5.183503] systemd[1]: Stopped File System Check on Root Device.
[    5.183607] systemd[1]: Stopped Journal Service.
[    5.185960] systemd[1]: Starting Journal Service...
[    5.187417] systemd[1]: Starting Load Kernel Modules...
[    5.188457] systemd[1]: Starting Generate network units from Kernel command line...
[    5.188541] systemd[1]: TPM2 PCR Machine ID Measurement was skipped because of an unmet condition check (ConditionPathExists=/sys/firmware/efi/efivars/StubPcrKernelImage-4a67b082-0a4c-41cf-b6c7-440b29bb8c4f).
[    5.189590] systemd[1]: Starting Remount Root and Kernel File Systems...
[    5.189707] systemd[1]: Repartition Root Disk was skipped because no trigger condition checks were met.
[    5.190749] systemd[1]: Starting Coldplug All udev Devices...
[    5.193962] systemd[1]: Activated swap /dev/mapper/rhel-swap.
[    5.195083] systemd[1]: Mounted Huge Pages File System.
[    5.195233] systemd[1]: Mounted POSIX Message Queue File System.
[    5.195349] systemd[1]: Mounted Kernel Debug File System.
[    5.195455] systemd[1]: Mounted Kernel Trace File System.
[    5.195845] systemd[1]: Finished Create List of Static Device Nodes.
[    5.196115] systemd[1]: modprobe@configfs.service: Deactivated successfully.
[    5.196217] systemd[1]: Finished Load Kernel Module configfs.
[    5.196393] systemd[1]: modprobe@drm.service: Deactivated successfully.
[    5.196487] systemd[1]: Finished Load Kernel Module drm.
[    5.196696] systemd[1]: modprobe@efi_pstore.service: Deactivated successfully.
[    5.196780] systemd[1]: Finished Load Kernel Module efi_pstore.
[    5.196940] systemd[1]: modprobe@fuse.service: Deactivated successfully.
[    5.197019] systemd[1]: Finished Load Kernel Module fuse.
[    5.197297] systemd[1]: Finished Read and set NIS domainname from /etc/sysconfig/network.
[    5.197579] systemd[1]: Finished Load Kernel Modules.
[    5.197826] systemd[1]: Finished Generate network units from Kernel command line.
[    5.198048] systemd[1]: Reached target Swaps.
[    5.199424] systemd[1]: Mounting FUSE Control File System...
[    5.200518] systemd[1]: Mounting Kernel Configuration File System...
[    5.201750] systemd[1]: Starting Apply Kernel Variables...
[    5.203704] systemd[1]: Finished Remount Root and Kernel File Systems.
[    5.203945] systemd[1]: Mounted FUSE Control File System.
[    5.204065] systemd[1]: Mounted Kernel Configuration File System.
[    5.204255] systemd[1]: Special handling of early boot iSCSI sessions was skipped because of an unmet condition check (ConditionDirectoryNotEmpty=/sys/class/iscsi_session).
[    5.204301] systemd[1]: OSTree Remount OS/ Bind Mounts was skipped because of an unmet condition check (ConditionKernelCommandLine=ostree).
[    5.204327] systemd[1]: First Boot Wizard was skipped because of an unmet condition check (ConditionFirstBoot=yes).
[    5.205575] systemd[1]: Rebuild Hardware Database was skipped because of an unmet condition check (ConditionNeedsUpdate=/etc).
[    5.205667] systemd[1]: Platform Persistent Storage Archival was skipped because of an unmet condition check (ConditionDirectoryNotEmpty=/sys/fs/pstore).
[    5.206894] systemd[1]: Starting Load/Save OS Random Seed...
[    5.206995] systemd[1]: Create System Users was skipped because no trigger condition checks were met.
[    5.208056] systemd[1]: Starting Create Static Device Nodes in /dev...
[    5.209425] systemd[1]: Started Journal Service.
[    5.217284] systemd-journald[779]: Received client request to flush runtime journal.
[    5.709442] IPMI message handler: version 39.2
[    5.732587] ipmi device interface
[    5.734681] intel_vsec 0000:00:0a.0: enabling device (0000 -> 0002)
[    5.747503] i801_smbus 0000:00:1f.4: SPD Write Disable is set
[    5.747566] i801_smbus 0000:00:1f.4: SMBus using PCI interrupt
[    5.748513] ipmi_si: IPMI System Interface driver
[    5.750904] ipmi_si dmi-ipmi-si.0: ipmi_platform: probing via SMBIOS
[    5.750910] ipmi_platform: ipmi_si: SMBIOS: io 0xcc0 regsize 1 spacing 1 irq 0
[    5.750915] ipmi_si: Adding SMBIOS-specified kcs state machine
[    5.764766] ipmi_si: Trying SMBIOS-specified kcs state machine at i/o address 0xcc0, slave address 0x20, irq 0
[    5.770336] i2c i2c-0: 2/2 memory slots populated (from DMI)
[    5.773971] i2c i2c-0: Successfully instantiated SPD at 0x50
[    5.775959] input: PC Speaker as /devices/platform/pcspkr/input/input8
[    5.798318] mei_me 0000:00:16.0: hbm: dma setup response: failure = 3 REJECTED
[    5.814576] cdc_ether 3-9.6:1.0 usb0: register 'cdc_ether' at usb-0000:00:14.0-9.6, CDC Ethernet Device, 8e:3b:4a:9a:b5:81
[    5.814710] usbcore: registered new interface driver cdc_ether
[    5.843742] iTCO_vendor_support: vendor-support=0
[    5.850416] RAPL PMU: API unit is 2^-32 Joules, 4 fixed counters, 655360 ms ovfl timer
[    5.850421] RAPL PMU: hw unit of domain pp0-core 2^-14 Joules
[    5.850423] RAPL PMU: hw unit of domain package 2^-14 Joules
[    5.850424] RAPL PMU: hw unit of domain pp1-gpu 2^-14 Joules
[    5.850425] RAPL PMU: hw unit of domain psys 2^-14 Joules
[    5.851659] iTCO_wdt iTCO_wdt: Found a Intel PCH TCO device (Version=6, TCOBASE=0x0400)
[    5.851820] iTCO_wdt iTCO_wdt: initialized. heartbeat=30 sec (nowayout=0)
[    5.857877] cdc_ether 3-9.6:1.0 enp0s20f0u9u6: renamed from usb0
[    5.864273] ipmi_si dmi-ipmi-si.0: IPMI message handler: Found new BMC (man_id: 0x004a66, prod_id: 0x070e, dev_id: 0x20)
[    6.053410] ipmi_si dmi-ipmi-si.0: IPMI kcs interface initialized
[    6.077953] ipmi_ssif: IPMI SSIF Interface driver
[    6.102133] intel_rapl_common: Found RAPL domain package
[    6.102139] intel_rapl_common: Found RAPL domain core
[    6.102141] intel_rapl_common: Found RAPL domain uncore
[    6.102144] intel_rapl_common: Found RAPL domain psys
[    6.155267] XFS (nvme0n1p2): Mounting V5 Filesystem 3e24f24a-46ae-430e-9e31-4646696c0920
[    6.155307] XFS (dm-2): Mounting V5 Filesystem 640ae256-f427-403d-a1ca-70b93e40c1cd
[    6.165278] XFS (dm-2): Ending clean mount
[    6.168104] XFS (nvme0n1p2): Ending clean mount
[    7.116804] NET: Registered PF_QIPCRTR protocol family
[    7.444329] Warning: Unmaintained driver is detected: ip_set
[   10.709020] tg3 0000:04:00.1 eno2: Link is up at 1000 Mbps, full duplex
[   10.709050] tg3 0000:04:00.1 eno2: Flow control is on for TX and on for RX
[   10.709053] tg3 0000:04:00.1 eno2: EEE is enabled
[   14.588832] block dm-0: the capability attribute has been deprecated.
[   14.694619] block nvme0n1: No UUID available providing old NGUID
[   27.174156] rfkill: input handler disabled
[   32.290586] rfkill: input handler enabled
[   34.718062] rfkill: input handler disabled
[   71.422530] bridge: filtering via arp/ip/ip6tables is no longer available by default. Update your scripts to load br_netfilter if you need this.
[   71.682778] Warning: Unmaintained driver is detected: nft_compat
[  107.944486] VFIO - User Level meta-driver version: 0.3
[  108.466946] tun: Universal TUN/TAP device driver, 1.6
[  108.468361] virbr0: port 1(vnet0) entered blocking state
[  108.468371] virbr0: port 1(vnet0) entered disabled state
[  108.468426] device vnet0 entered promiscuous mode
[  108.469064] virbr0: port 1(vnet0) entered blocking state
[  108.469067] virbr0: port 1(vnet0) entered listening state
[  110.512678] virbr0: port 1(vnet0) entered learning state
[  112.560638] virbr0: port 1(vnet0) entered forwarding state
[  112.560655] virbr0: topology change detected, propagating
[  161.705729] virbr0: port 1(vnet0) entered disabled state
[  161.706208] device vnet0 left promiscuous mode
[  161.706226] virbr0: port 1(vnet0) entered disabled state
[  162.172362] nvme nvme1: pci function 0000:03:00.0
[  162.226562] nvme nvme1: 14/0/0 default/read/poll queues
[  162.230637]  nvme1n1:
[  220.271294] virbr0: port 1(vnet1) entered blocking state
[  220.271305] virbr0: port 1(vnet1) entered disabled state
[  220.271377] device vnet1 entered promiscuous mode
[  220.271738] virbr0: port 1(vnet1) entered blocking state
[  220.271742] virbr0: port 1(vnet1) entered listening state
[  222.319586] virbr0: port 1(vnet1) entered learning state
[  224.367567] virbr0: port 1(vnet1) entered forwarding state
[  224.367585] virbr0: topology change detected, propagating
[  238.251210] pcieport 0000:00:01.0: AER: Multiple Uncorrectable (Non-Fatal) error message received from 0000:01:00.0
[  238.251243] vfio-pci 0000:01:00.0: PCIe Bus Error: severity=Uncorrectable (Non-Fatal), type=Transaction Layer, (Requester ID)
[  238.251252] vfio-pci 0000:01:00.0:   device [14e4:16d8] error status/mask=00100000/00400000
[  238.251258] vfio-pci 0000:01:00.0:    [20] UnsupReq               (First)
[  238.251263] vfio-pci 0000:01:00.0: AER:   TLP Header: 60000001 0000000f 00000040 18300000
[  238.251268] vfio-pci 0000:01:00.0: AER:   Error of this Agent is reported first
[  238.251279] vfio-pci 0000:01:00.1: PCIe Bus Error: severity=Uncorrectable (Non-Fatal), type=Transaction Layer, (Requester ID)
[  238.251283] vfio-pci 0000:01:00.1:   device [14e4:16d8] error status/mask=00100000/00400000
[  238.251287] vfio-pci 0000:01:00.1:    [20] UnsupReq               (First)
[  238.251290] vfio-pci 0000:01:00.1: AER:   TLP Header: 60000001 0000000f 00000040 18300000
[  238.251463] pcieport 0000:00:01.0: AER: device recovery successful
[  238.251536] pcieport 0000:00:01.0: AER: device recovery successful
