ipsec status
000 using kernel interface: xfrm
000  
000 interface lo UDP [::1]:4500
000 interface lo UDP [::1]:500
000 interface lo UDP 127.0.0.1:4500
000 interface lo UDP 127.0.0.1:500
000 interface ovn-k8s-mp0 UDP 10.254.20.2:4500
000 interface ovn-k8s-mp0 UDP 10.254.20.2:500
000 interface br-ex UDP 10.17.82.86:4500
000 interface br-ex UDP 10.17.82.86:500
000 interface br-ex UDP 169.254.0.2:4500
000 interface br-ex UDP 169.254.0.2:500
000  
000 fips mode=disabled;
000 SElinux=disabled
000 seccomp=disabled
000  
000 config setup options:
000  
000 configdir=/etc, configfile=/etc/ipsec.conf, secrets=/etc/ipsec.secrets, ipsecdir=/etc/ipsec.d
000 nssdir=/var/lib/ipsec/nss, dumpdir=/run/pluto, statsbin=unset
000 dnssec-rootkey-file=/var/lib/unbound/root.key, dnssec-trusted=<unset>
000 sbindir=/usr/sbin, libexecdir=/usr/libexec/ipsec
000 pluto_version=4.15, pluto_vendorid=OE-Libreswan-4.15, audit-log=yes
000 nhelpers=-1, uniqueids=yes, dnssec-enable=yes, logappend=yes, logip=yes, shuntlifetime=900s, xfrmlifetime=30s
000 ddos-cookies-threshold=25000, ddos-max-halfopen=50000, ddos-mode=auto, ikev1-policy=accept
000 ikebuf=0, msg_errqueue=yes, crl-strict=no, crlcheckinterval=0, listen=<any>, nflog-all=0
000 ocsp-enable=no, ocsp-strict=no, ocsp-timeout=2, ocsp-uri=<unset>
000 ocsp-trust-name=<unset>
000 ocsp-cache-size=1000, ocsp-cache-min-age=3600, ocsp-cache-max-age=86400, ocsp-method=get
000 global-redirect=no, global-redirect-to=<unset>
000 secctx-attr-type=32001
000 debug:
000  
000 nat-traversal=yes, keep-alive=20, nat-ikeport=4500
000 virtual-private (%priv):
000  
000 Kernel algorithms supported:
000  
000 algorithm ESP encrypt: name=3DES_CBC, keysizemin=192, keysizemax=192
000 algorithm ESP encrypt: name=AES_CBC, keysizemin=128, keysizemax=256
000 algorithm ESP encrypt: name=AES_CCM_12, keysizemin=128, keysizemax=256
000 algorithm ESP encrypt: name=AES_CCM_16, keysizemin=128, keysizemax=256
000 algorithm ESP encrypt: name=AES_CCM_8, keysizemin=128, keysizemax=256
000 algorithm ESP encrypt: name=AES_CTR, keysizemin=128, keysizemax=256
000 algorithm ESP encrypt: name=AES_GCM_12, keysizemin=128, keysizemax=256
000 algorithm ESP encrypt: name=AES_GCM_16, keysizemin=128, keysizemax=256
000 algorithm ESP encrypt: name=AES_GCM_8, keysizemin=128, keysizemax=256
000 algorithm ESP encrypt: name=CAMELLIA_CBC, keysizemin=128, keysizemax=256
000 algorithm ESP encrypt: name=CHACHA20_POLY1305, keysizemin=256, keysizemax=256
000 algorithm ESP encrypt: name=NULL, keysizemin=0, keysizemax=0
000 algorithm ESP encrypt: name=NULL_AUTH_AES_GMAC, keysizemin=128, keysizemax=256
000 algorithm AH/ESP auth: name=AES_CMAC_96, key-length=128
000 algorithm AH/ESP auth: name=AES_XCBC_96, key-length=128
000 algorithm AH/ESP auth: name=HMAC_MD5_96, key-length=128
000 algorithm AH/ESP auth: name=HMAC_SHA1_96, key-length=160
000 algorithm AH/ESP auth: name=HMAC_SHA2_256_128, key-length=256
000 algorithm AH/ESP auth: name=HMAC_SHA2_256_TRUNCBUG, key-length=256
000 algorithm AH/ESP auth: name=HMAC_SHA2_384_192, key-length=384
000 algorithm AH/ESP auth: name=HMAC_SHA2_512_256, key-length=512
000 algorithm AH/ESP auth: name=NONE, key-length=0
000  
000 IKE algorithms supported:
000  
000 algorithm IKE encrypt: v1id=5, v1name=OAKLEY_3DES_CBC, v2id=3, v2name=3DES, blocksize=8, keydeflen=192
000 algorithm IKE encrypt: v1id=8, v1name=OAKLEY_CAMELLIA_CBC, v2id=23, v2name=CAMELLIA_CBC, blocksize=16, keydeflen=128
000 algorithm IKE encrypt: v1id=-1, v1name=n/a, v2id=20, v2name=AES_GCM_C, blocksize=16, keydeflen=128
000 algorithm IKE encrypt: v1id=-1, v1name=n/a, v2id=19, v2name=AES_GCM_B, blocksize=16, keydeflen=128
000 algorithm IKE encrypt: v1id=-1, v1name=n/a, v2id=18, v2name=AES_GCM_A, blocksize=16, keydeflen=128
000 algorithm IKE encrypt: v1id=13, v1name=OAKLEY_AES_CTR, v2id=13, v2name=AES_CTR, blocksize=16, keydeflen=128
000 algorithm IKE encrypt: v1id=7, v1name=OAKLEY_AES_CBC, v2id=12, v2name=AES_CBC, blocksize=16, keydeflen=128
000 algorithm IKE encrypt: v1id=-1, v1name=n/a, v2id=28, v2name=CHACHA20_POLY1305, blocksize=16, keydeflen=256
000 algorithm IKE PRF: name=HMAC_MD5, hashlen=16
000 algorithm IKE PRF: name=HMAC_SHA1, hashlen=20
000 algorithm IKE PRF: name=HMAC_SHA2_256, hashlen=32
000 algorithm IKE PRF: name=HMAC_SHA2_384, hashlen=48
000 algorithm IKE PRF: name=HMAC_SHA2_512, hashlen=64
000 algorithm IKE PRF: name=AES_XCBC, hashlen=16
000 algorithm IKE DH Key Exchange: name=MODP1536, bits=1536
000 algorithm IKE DH Key Exchange: name=MODP2048, bits=2048
000 algorithm IKE DH Key Exchange: name=MODP3072, bits=3072
000 algorithm IKE DH Key Exchange: name=MODP4096, bits=4096
000 algorithm IKE DH Key Exchange: name=MODP6144, bits=6144
000 algorithm IKE DH Key Exchange: name=MODP8192, bits=8192
000 algorithm IKE DH Key Exchange: name=DH19, bits=512
000 algorithm IKE DH Key Exchange: name=DH20, bits=768
000 algorithm IKE DH Key Exchange: name=DH21, bits=1056
000 algorithm IKE DH Key Exchange: name=DH31, bits=256
000  
000 stats db_ops: {curr_cnt, total_cnt, maxsz} :context={0,0,0} trans={0,0,0} attrs={0,0,0} 
000  
000 Connection list:
000  
000 "submariner-cable-rdr-blue-site-svl-1-10-17-109-163-0-0": 242.1.0.0/16===10.17.82.86:4500[+S?C]...10.17.109.163:4500[+S?C]===242.0.0.0/16; erouted; eroute owner: #5
000 "submariner-cable-rdr-blue-site-svl-1-10-17-109-163-0-0":     oriented; my_ip=unset; their_ip=unset; my_updown=ipsec _updown;
000 "submariner-cable-rdr-blue-site-svl-1-10-17-109-163-0-0":   xauth us:none, xauth them:none,  my_username=[any]; their_username=[any]
000 "submariner-cable-rdr-blue-site-svl-1-10-17-109-163-0-0":   our auth:secret, their auth:secret, our autheap:none, their autheap:none;
000 "submariner-cable-rdr-blue-site-svl-1-10-17-109-163-0-0":   modecfg info: us:none, them:none, modecfg policy:push, dns:unset, domains:unset, cat:unset;
000 "submariner-cable-rdr-blue-site-svl-1-10-17-109-163-0-0":   sec_label:unset;
000 "submariner-cable-rdr-blue-site-svl-1-10-17-109-163-0-0":   ike_life: 28800s; ipsec_life: 28800s; ipsec_max_bytes: 2^63B; ipsec_max_packets: 2^63; replay_window: 128; rekey_margin: 540s; rekey_fuzz: 100%; keyingtries: 0;
000 "submariner-cable-rdr-blue-site-svl-1-10-17-109-163-0-0":   retransmit-interval: 500ms; retransmit-timeout: 60s; iketcp:no; iketcp-port:4500;
000 "submariner-cable-rdr-blue-site-svl-1-10-17-109-163-0-0":   initial-contact:no; cisco-unity:no; fake-strongswan:no; send-vendorid:no; send-no-esp-tfc:no;
000 "submariner-cable-rdr-blue-site-svl-1-10-17-109-163-0-0":   policy: IKEv2+PSK+ENCRYPT+TUNNEL+UP;
000 "submariner-cable-rdr-blue-site-svl-1-10-17-109-163-0-0":   v2-auth-hash-policy: none;
000 "submariner-cable-rdr-blue-site-svl-1-10-17-109-163-0-0":   conn_prio: 16,16; interface: br-ex; metric: 0; mtu: unset; sa_prio:auto; sa_tfc:none;
000 "submariner-cable-rdr-blue-site-svl-1-10-17-109-163-0-0":   nflog-group: unset; mark: unset; vti-iface:unset; vti-routing:no; vti-shared:no; nic-offload:auto;
000 "submariner-cable-rdr-blue-site-svl-1-10-17-109-163-0-0":   our idtype: ID_IPV4_ADDR; our id=10.17.82.86; their idtype: ID_IPV4_ADDR; their id=10.17.109.163
000 "submariner-cable-rdr-blue-site-svl-1-10-17-109-163-0-0":   liveness: active; dpdaction:hold; dpddelay:30s; retransmit-timeout:60s
000 "submariner-cable-rdr-blue-site-svl-1-10-17-109-163-0-0":   nat-traversal: encaps:no; keepalive:20s
000 "submariner-cable-rdr-blue-site-svl-1-10-17-109-163-0-0":   newest IKE SA: #4; newest IPsec SA: #5; conn serial: $1;
000 "submariner-cable-rdr-blue-site-svl-1-10-17-109-163-0-0":   IKEv2 algorithm newest: AES_GCM_16_256-HMAC_SHA2_512-MODP2048
000 "submariner-cable-rdr-blue-site-svl-1-10-17-109-163-0-0":   ESP algorithm newest: AES_GCM_16_256-NONE; pfsgroup=<N/A>
000  
000 Total IPsec connections: loaded 1, active 1
000  
000 State Information: DDoS cookies not required, Accepting new IKE connections
000 IKE SAs: total(1), half-open(0), open(0), authenticated(1), anonymous(0)
000 IPsec SAs: total(1), authenticated(1), anonymous(0)
000  
000 #4: "submariner-cable-rdr-blue-site-svl-1-10-17-109-163-0-0":4500 STATE_V2_ESTABLISHED_IKE_SA (established IKE SA); REKEY in 23426s; REPLACE in 23696s; newest; idle;
000 #5: "submariner-cable-rdr-blue-site-svl-1-10-17-109-163-0-0":4500 STATE_V2_ESTABLISHED_CHILD_SA (established Child SA); LIVENESS in 26s; REKEY in 23426s; REPLACE in 23696s; newest; eroute owner; IKE SA #4; idle;
000 #5: "submariner-cable-rdr-blue-site-svl-1-10-17-109-163-0-0" esp.67572fe7@10.17.109.163 esp.e1c1aef8@10.17.82.86 tun.0@10.17.109.163 tun.0@10.17.82.86 Traffic: ESPin=14MB ESPout=14MB ESPmax=2^63B 
000  
000 Bare Shunt list:
000